==========
NuttX RTOS
==========

What is NuttX?
--------------

`NuttX <https://nuttx.apache.org/>`__ is a mature and secure real-time
operating system (RTOS) with an emphasis on technical standards
compliance and small size. It is scalable from 8-bit to 64-bit
microcontrollers and microprocessors and compliant with the Portable
Operating System Interface (POSIX) and the American National Standards
Institute (ANSI) standards and with many Linux-like subsystems. The best
way to think about NuttX is to think of it as a small Unix/Linux for
microcontrollers.

Highlights of NuttX
~~~~~~~~~~~~~~~~~~~

-  **Small** - Fits and runs in microcontrollers as small as 32 kB Flash
   and 8 kB of RAM.
-  **Compliant** - Strives to be as compatible as possible with POSIX
   and Linux.
-  **Versatile** - Supports many architectures (ARM, ARM Thumb, AVR,
   MIPS, OpenRISC, RISC-V 32-bit and 64-bit, RX65N, x86-64, Xtensa,
   Z80/Z180, etc.).
-  **Modular** - Its modular design allows developers to select only
   what really matters and use modules to include new features.
-  **Popular** - NuttX is used by many companies around the world.
   Probably you already used a product with NuttX without knowing it was
   running NuttX.
-  **Predictable** - NuttX is a preemptible Realtime kernel, so you can
   use it to create predictable applications for realtime control.

--------------

Why NuttX + LVGL?
-----------------

Although NuttX has its own graphic library called
`NX <https://cwiki.apache.org/confluence/pages/viewpage.action?pageId=139629474>`__,
LVGL is a good alternative because users could find more eye-candy demos
and they can reuse code from previous projects. LVGL is an
`Object-Oriented Component
Based <https://blog.lvgl.io/2018-12-13/extend-lvgl-objects>`__
high-level GUI library, that could fit very well for a RTOS with
advanced features like NuttX. LVGL is implemented in C and its APIs are
in C.

Here are some advantages of using LVGL in NuttX
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

-  Develop GUI in Linux first and when it is done just compile it for
   NuttX. Nothing more, no wasting of time.
-  Usually, GUI development for low level RTOS requires multiple
   iterations to get things right, where each iteration consists of
   **``Change code`` > ``Build`` > ``Flash`` > ``Run``**. Using LVGL,
   Linux and NuttX you can reduce this process and just test everything
   on your computer and when it is done, compile it on NuttX and that is
   it.

NuttX + LVGL could be used for
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

-  GUI demos to demonstrate your board graphics capacities.
-  Fast prototyping GUI for MVP (Minimum Viable Product) presentation.
-  visualize sensor data directly and easily on the board without using
   a computer.
-  Final products with a GUI without a touchscreen (i.e. 3D Printer
   Interface using Rotary Encoder to Input data).
-  Final products with a touchscreen (and all sorts of bells and
   whistles).

--------------

How to get started with NuttX and LVGL?
---------------------------------------

There are many boards in the `NuttX
mainline <https://github.com/apache/incubator-nuttx>`__ with support for
LVGL. Let's use the
`STM32F429IDISCOVERY <https://www.st.com/en/evaluation-tools/32f429idiscovery.html>`__
as an example because it is a very popular board.

First you need to install the pre-requisites on your system
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

Let's use the `Windows Subsystem for
Linux <https://acassis.wordpress.com/2018/01/10/how-to-build-nuttx-on-windows-10/>`__

.. code:: shell

   $ sudo apt-get install automake bison build-essential flex gcc-arm-none-eabi gperf git libncurses5-dev libtool libusb-dev libusb-1.0.0-dev pkg-config kconfig-frontends openocd

Now let's create a workspace to save our files
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

.. code:: shell

   $ mkdir ~/nuttxspace
   $ cd ~/nuttxspace

Clone the NuttX and Apps repositories:
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

.. code:: shell

   $ git clone https://github.com/apache/incubator-nuttx nuttx
   $ git clone https://github.com/apache/incubator-nuttx-apps apps

Configure NuttX to use the stm32f429i-disco board and the LVGL Demo
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

.. code:: shell

   $ ./tools/configure.sh stm32f429i-disco:lvgl
   $ make

If everything went fine you should have now the file ``nuttx.bin`` to
flash on your board:

.. code:: shell

   $ ls -l nuttx.bin
   -rwxrwxr-x 1 alan alan 287144 Jun 27 09:26 nuttx.bin

Flashing the firmware in the board using OpenOCD:
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~

.. code:: shell

   $ sudo openocd -f interface/stlink-v2.cfg -f target/stm32f4x.cfg -c init -c "reset halt" -c "flash write_image erase nuttx.bin 0x08000000"

Reset the board and using the 'NSH>' terminal start the LVGL demo:

.. code:: shell

   nsh> lvgldemo

Where can I find more information?
----------------------------------

-  This blog post: `LVGL on
   LPCXpresso54628 <https://acassis.wordpress.com/2018/07/19/running-nuttx-on-lpcxpresso54628-om13098/>`__
-  NuttX mailing list: `Apache NuttX Mailing
   List <http://nuttx.incubator.apache.org/community/>`__
