Skip to content

Register now for

# YOLOv10 vs PP-YOLOE+: A Technical Comparison for Object Detection

Choosing the optimal object detection model is crucial for balancing accuracy, speed, and computational resources in computer vision tasks. This page offers a technical comparison between YOLOv10, the latest advancement from Tsinghua University integrated into the Ultralytics ecosystem, and PP-YOLOE+, a high-accuracy model from Baidu. We analyze their architectures, performance, and applications to guide your decision, highlighting the advantages of YOLOv10.

## YOLOv10: End-to-End Efficiency

Ultralytics YOLOv10 is a groundbreaking iteration in the YOLO series, focusing on true real-time, end-to-end object detection. Developed by researchers at Tsinghua University, its primary innovation is eliminating the need for Non-Maximum Suppression (NMS) post-processing, which significantly reduces inference latency and simplifies deployment pipelines.

Technical Details:

- Authors: Ao Wang, Hui Chen, Lihao Liu, et al.
- Organization: Tsinghua University
- Date: 2024-05-23
- Arxiv Link: https://arxiv.org/abs/2405.14458
- GitHub Link: https://github.com/THU-MIG/yolov10
- Docs Link: https://docs.ultralytics.com/models/yolov10/

### Key Features and Architecture

- NMS-Free Training: YOLOv10 employs consistent dual assignments during training, which allows it to generate clean predictions without requiring NMS at inference time. This is a major advantage for real-time applications where every millisecond of latency counts.
- Holistic Efficiency-Accuracy Driven Design: The model architecture has been comprehensively optimized to reduce computational redundancy. This includes innovations like a lightweight classification head and spatial-channel decoupled downsampling, which enhance model capability while minimizing resource usage.
- Anchor-Free Detection: Like many modern detectors, it uses an anchor-free approach, simplifying the architecture and improving generalization across different object sizes and aspect ratios.
- Ultralytics Ecosystem Integration: As an Ultralytics-supported model, YOLOv10 benefits from a robust and well-maintained ecosystem. This provides users with a streamlined experience through a simple Python API, extensive documentation, efficient training processes with readily available pre-trained weights, and seamless integration with Ultralytics HUB for end-to-end project management.

### Use Cases

- Real-time Video Analytics: Ideal for applications like autonomous driving, robotics, and high-speed surveillance where low inference latency is critical.
- Edge Deployment: The smaller variants (YOLOv10n/s) are highly optimized for resource-constrained devices such as NVIDIA Jetson and Raspberry Pi, making advanced AI accessible on the edge.
- High-Accuracy Applications: Larger models provide state-of-the-art precision for demanding tasks like medical image analysis or detailed quality inspection in manufacturing.

### Strengths and Weaknesses

Strengths:

- Superior speed and efficiency due to its NMS-free design.
- Excellent balance between speed and accuracy across all model sizes.
- Highly scalable, offering variants from Nano (N) to Extra-large (X).
- Lower memory requirements and efficient training.
- Ease of use and strong support within the well-maintained Ultralytics ecosystem.

Weaknesses:

- As a newer model, the community outside of the Ultralytics ecosystem is still growing.
- Achieving peak performance may require hardware-specific optimizations like TensorRT.

Learn more about YOLOv10

## PP-YOLOE+: High Accuracy in the PaddlePaddle Framework

PP-YOLOE+, developed by Baidu, is an enhanced version of PP-YOLOE that focuses on achieving high accuracy while maintaining efficiency. It is a key model within the PaddlePaddle deep learning framework.

Technical Details:

- Authors: PaddlePaddle Authors
- Organization: Baidu
- Date: 2022-04-02
- Arxiv Link: https://arxiv.org/abs/2203.16250
- GitHub Link: https://github.com/PaddlePaddle/PaddleDetection/
- Docs Link: https://github.com/PaddlePaddle/PaddleDetection/blob/release/2.8.1/configs/ppyoloe/README.md

### Key Features and Architecture

- Anchor-Free Design: Like YOLOv10, it is an anchor-free detector, which simplifies the detection head and reduces the number of hyperparameters to tune.
- CSPRepResNet Backbone: It utilizes a backbone that combines principles from CSPNet and RepResNet for powerful feature extraction.
- Advanced Loss and Head: The model incorporates Varifocal Loss and an efficient ET-Head to improve the alignment between classification and localization tasks.

### Use Cases

- Industrial Quality Inspection: Its high accuracy makes it suitable for detecting subtle defects in manufacturing lines.
- Smart Retail: Can be used for applications like automated inventory management and customer behavior analysis.
- Recycling Automation: Effective at identifying different materials for automated sorting systems.

### Strengths and Weaknesses

Strengths:

- Achieves high accuracy, especially with its larger model variants.
- Well-integrated within the PaddlePaddle ecosystem.
- Efficient anchor-free design.

Weaknesses:

- Primarily optimized for the PaddlePaddle framework, which can create a steep learning curve and integration challenges for developers using other frameworks like PyTorch.
- Community support and available resources may be less extensive compared to the vast ecosystem surrounding Ultralytics models.
- Larger models have significantly more parameters than YOLOv10 equivalents, leading to higher computational costs.

Learn more about PP-YOLOE+

## Performance Analysis: Speed, Accuracy, and Efficiency

Model | size (pixels) | mAPval 50-95 | Speed CPU ONNX (ms) | Speed T4 TensorRT10 (ms) | params (M) | FLOPs (B)
--- | --- | --- | --- | --- | --- | ---
YOLOv10n | 640 | 39.5 | - | 1.56 | 2.3 | 6.7
YOLOv10s | 640 | 46.7 | - | 2.66 | 7.2 | 21.6
YOLOv10m | 640 | 51.3 | - | 5.48 | 15.4 | 59.1
YOLOv10b | 640 | 52.7 | - | 6.54 | 24.4 | 92.0
YOLOv10l | 640 | 53.3 | - | 8.33 | 29.5 | 120.3
YOLOv10x | 640 | 54.4 | - | 12.2 | 56.9 | 160.4
PP-YOLOE+t | 640 | 39.9 | - | 2.84 | 4.85 | 19.15
PP-YOLOE+s | 640 | 43.7 | - | 2.62 | 7.93 | 17.36
PP-YOLOE+m | 640 | 49.8 | - | 5.56 | 23.43 | 49.91
PP-YOLOE+l | 640 | 52.9 | - | 8.36 | 52.2 | 110.07
PP-YOLOE+x | 640 | 54.7 | - | 14.3 | 98.42 | 206.59

The performance metrics reveal a clear distinction between the two models. YOLOv10 consistently demonstrates superior parameter and computational efficiency. For instance, YOLOv10-L achieves a comparable 53.3% mAP to PP-YOLOE+-l's 52.9% mAP, but with nearly 44% fewer parameters (29.5M vs 52.2M). This trend continues to the largest models, where YOLOv10-X reaches 54.4% mAP with 56.9M parameters, while PP-YOLOE+-x requires a massive 98.42M parameters to achieve a slightly higher 54.7% mAP.

In terms of speed, YOLOv10's NMS-free architecture gives it a distinct advantage, especially for real-time deployment. The smallest model, YOLOv10-N, boasts an impressive 1.56ms latency, making it a top choice for edge AI applications. While PP-YOLOE+ can achieve high accuracy, it often comes at the cost of a much larger model size and higher computational demand, making YOLOv10 the more efficient and practical choice for a wider range of deployment scenarios.

## Conclusion: Why YOLOv10 is the Recommended Choice

While both YOLOv10 and PP-YOLOE+ are powerful object detectors, YOLOv10 emerges as the superior choice for the vast majority of developers and researchers. Its groundbreaking NMS-free architecture provides a significant advantage in real-world applications by reducing latency and simplifying the deployment pipeline.

The key advantages of YOLOv10 include:

- Unmatched Efficiency: It delivers a better speed-accuracy trade-off, achieving competitive mAP scores with significantly fewer parameters and FLOPs than PP-YOLOE+. This translates to lower computational costs and the ability to run on less powerful hardware.
- True End-to-End Detection: By eliminating the NMS bottleneck, YOLOv10 is faster and easier to deploy, especially in latency-sensitive environments like robotics and autonomous systems.
- Superior User Experience: Integrated into the Ultralytics ecosystem, YOLOv10 offers unparalleled ease of use, comprehensive documentation, active community support, and straightforward training and export workflows. This drastically reduces development time and effort.

PP-YOLOE+ is a strong performer in terms of raw accuracy but is largely confined to the PaddlePaddle ecosystem. Its larger model sizes and framework dependency make it a less flexible and more resource-intensive option compared to the highly optimized and user-friendly YOLOv10. For projects that demand a balance of high performance, efficiency, and ease of development, YOLOv10 is the clear winner.

## Explore Other Models

For those interested in exploring other state-of-the-art models, Ultralytics provides detailed comparisons for a wide range of architectures. Consider looking into YOLOv8 for its proven versatility across multiple vision tasks, or check out our comparisons with models like RT-DETR and YOLOv9 to find the perfect fit for your project.

📅 Created 1 year ago ✏️ Updated 1 month ago

## Comments