# Please note that this is only a sample, we recommend you to change it to fit
# your needs.
# You should override this file using BR2_PACKAGE_RPI_FIRMWARE_CONFIG_FILE.
# See http://buildroot.org/manual.html#rootfs-custom
# and http://elinux.org/RPiconfig for a description of config.txt syntax

start_file=start.elf
fixup_file=fixup.dat

kernel=zImage

# To use an external initramfs file
#initramfs rootfs.cpio.gz

# Disable overscan assuming the display supports displaying the full resolution
# If the text shown on the screen disappears off the edge, comment this out
disable_overscan=1

# How much memory in MB to assign to the GPU on Pi models having
# 256, 512 or 1024 MB total memory
gpu_mem_256=100
gpu_mem_512=100
gpu_mem_1024=100

# Enable UART0 for serial console on ttyAMA0
dtoverlay=miniuart-bt

# enable autoprobing of Bluetooth driver without need of hciattach/btattach
dtparam=krnbt=on
