Update Release

02.27.2026 - GUI Updates + Small Bug Fix

  1. Added Zoom in/out Option for Partition Table via CTRL+ Mouse Scroll Wheel (Requested by md hasan)
 
  2. Added Zoom in/out Option for Hex Editor via CTRL+ Mouse Scroll Wheel

  3. Fixed Hex Editor Save and Auto-Save function

  4. Improved Hex Editor Cell Range selection



02.26.2026 - Realtime Hex Editor, Themes, Image Viewer, Speed Graph and 2026 Flashing Updates

  1. Added Realtime Hex Editor for direct partition editing
     * Partitions larger than 1GB will not have the auto-backup feature. Manually SAVE file using the Save Button.
     * Partitions smaller then 1GB will have the auto-backup feature.

  2. Added Application Theme selection (Night, Graphite, Light)

  3. Added Image Viewer

  4. Added Line Graph for showing Transfer Speed Logs (Minimum, Maximum, Average and Current Speed)

  5. Added Country/Provider Variant selection for Vivo factory files (MTK, Qualcomm and SPD/Unisoc) (Requested by D Stealth Warrior)

  6. Added full display of all files used when a partition is flashed with more than 1 file (Requested by D Stealth Warrior)

  7. Added Qualcomm rawprogram.xml type selection (unsparsed, no_qcn etc...)
     * This will select the correct combination of XML files based on the first file selected by the user

  8. Added new option "Restart USB" when closing application
     * This will automatically Cycle the used USB Port in case a stall has occurred
     * The application with automatically restart with the newly refreshed USB Port

  9. Bug fixed for Android Verified Boot (AVB) Process on UFS Qualcomm Phones

 10. Bug fixed for flashing multi-sparsed files

 11. Bug fixed for Factory Provisioning Micron UFS 4.0 and UFS 4.1

 12. Bug fixed for MTK MT6833 preloader loading (Reported by Samim Vai)

 13. Bug fixed for MTK MT6768 preloader loading via scatter.txt (Reported by Giovanni Lucas Da Paz)




02.11.2026 – Moving Partitions and New MTK Dimensity 9500 Support

  1. Added Scatter TXT and XML support for MTK Dimensity 9500 UFS provisioning.

  2. Added Factory Firmware flashing for MTK Dimensity 9500.

  3. Added AVB preloader verification for MTK Dimensity 9500.

  4. Added "Safe Connect" option when holding down the Shift key during UFS/eMMC IC detection.

  5. Bug fix for reading Vivo, iQOO, and Jovi information on eMMC (Thanks to hello-firmware.com).

  6. Added GPT Partition Move **** THIS WILL DAMAGE USERDATA ****
  * Moves partition address and data away from Write Protected areas.
  * A single partition or multiple partitions can be moved together.
  * This damages userdata. Userdata needs to be formatted or flashed with stock file.

  7. Added DEFLATE and MicroLZMA compression support for EROFS.

  8. Added AUTO 1 and AUTO 2 options for TXN setting.

  9. Minor bug fixes and improvements.

  *** Thank you to YunYi and Mr.UPROM! for providing Dimensity 9500 dumps 



01.31.2026 - Multi-Programming Edition

  *** Box Firmware Update is Recommended before using this updated software ***

  1. Added support for upto 32 F64 boxes connected together in 1 computer.
     * Each F64 box should have it's own FOLDER and Special Multi-Programming Edition EXE
     * An external 5V (1000 mA) USB C External power source should be used for each F64 box
     * Your computer should have enough resources to handle the bandwidth and power demands
     * You must use the Multi-Programming Edition EXE for this feature

  2. RPMB Key Read for NON-SECURE DL6DAB : KMDL6001DA-B425
     * This feature only works after eMMC FFU + Full Factory Reset
     * Do not use this feature on SM-A055F BIT 10 and BIT 11
     * Do not use this on a phone that does not provision the RPMB of a blank eMMC
     * Do not use this if you do not understand the 3 statements above

  3. Added support for Oppo, Realme and Oneplus 2026 Official Firmware Files

  4. Added support for loading single partition file automatically from the same folder

  5. Added support for Unisoc PAC and XML files for UFS Provision.

  6. Added support for MTK Scatter XML files for UFS Provision.

  7. Automatically skips Unisoc RF/IMEI partitions loaded from Factory Firmware Files.

  8. Improved Android Factory Reset for Oppo, Realme, Vivo and iQOO

  9. Vivo, iQOO, Jovi Read Device Info Added (Thanks to hello-firmware.com)

 10. Fixed Security Patch Version Reading for A16 Vivo, iQOO, Jovi phones.

 11. Added TXN option "AUTO" which automatically switches between TXN values
  
 12. Added New Samsung eMMC FFU:
     RP64AB : KMRP60014A-B614 (Contributed by 0x9k (Circuit Knight X))

 13. Behind the scene bug fixes (Thanks, Mr.UPROM!)

 14. SkHynix eMMC detection bug improvements (Thanks to hello-firmware.com)  



Update Release

12.17.2025

  *** Box Firmware Update is Recommended before using this updated software ***

1. Added support for Sandisk/Western Digital Corporation UFS 4.0 & UFS 4.1 (requires ASIC Firmware 12.10.2025) 

2. Added support for Samsung UFS 4.1 via 270mV (Signal Booster) setting only 

3. Added Android Boot Unpack + Decompress (In Developer Tools)

4. Added Android Boot Pack + Compress (In Developer Tools)

5. Sparse Image Flashing Improved 

6. Added support for vbmeta with empty Authentication Block in AVB Task. 

7. Fixed OCDT Partition Flashing in Oppo, Realme and OnePlus

8. Added support for ALL Google PIXEL Phones GPT Authoring via Factory Bootloader files 

9. Added support for ALL Google PIXEL Phones flashing via flash-all.bat or flash-all.sh
   * As of the moment, you can use this to repair dead boot on ALL Google PIXEL phones with the exception of Pixel C (2015)

     Pixel 10 Pro XL - mustang
     Pixel 10 Pro Fold - rango 
     Pixel 10 Pro - blazer
     Pixel 10 - frankel
     Pixel 9a - tegu
     Pixel 9 Pro XL - komodo
     Pixel 9 Pro Fold - comet
     Pixel 9 Pro - caiman
     Pixel 9 - tokay
     Pixel 8a - akita
     Pixel 8 Pro - husky
     Pixel 8 - shiba
     Pixel Fold - felix
     Pixel Tablet - tangorpro
     Pixel 7A - lynx
     Pixel 7 Pro - cheetah
     Pixel 7 - panther
     Pixel 6a - bluejay
     Pixel 6 Pro - raven
     Pixel 6 - oriole
     Pixel 5a - barbet
     Pixel 5 - redfin
     Pixel 4a (5G) - bramble
     Pixel 4a - sunfish
     Pixel 4 XL - coral
     Pixel 4 - flame
     Pixel 3a XL - bonito
     Pixel 3a - sargo
     Pixel 3 XL - crosshatch
     Pixel 3 - blueline
     Pixel 2 XL - taimen
     Pixel 2 - walleye
     Pixel XL - marlin
     Pixel - sailfish

10. Added New Samsung eMMC FFU:
   
   *** These Firmwares are fully encrypted and they are NOT SUPPORTED for Smart Patches and RPMB Key Read ***
       (You can still use these firmwares for eMMC Health, RPMB Cleaning and for fixing dead eMMC 00000)
  
     DL6DAB : KMDL6001DA-B425 (Created by X-Shadow)
     DRTE42 : KLMDG2RCTE-B041 (Created by X-Shadow)

    



Update Releases

11.27.2025 - Software Maintenance Update

1. Reverted eMMC ISP Detection to a previous version

2. Added NEW Mi Master Boot Record Support for eMMC and UFS

3. Added Support for GPT Provision via Qualcomm Partition External (XML) files

4. Added Support for Loading files via Qualcomm Partition External (XML) files

5. Added Support for GPT Provision via Qualcomm rawprogram (XML) files (rawprogram0.xml, rawprogram1.xml etc...);
   *** Warning: Use this as a last option only if gpt_main0.bin, gpt_main1.bin etc files are not available

6. Oppo, Realme and OnePlus Factory Flashing Improvement
   * Always use correct Project ID

7. Oppo, Realme and OnePlus Project ID Detection

8. Added Android Verified Boot Function
   * You can learn about this function here:
     https://source.android.com/docs/security/features/verifiedboot 
   * Supports AVB versions 1.1.0, 1.2.0 and 1.3.0
   * Supports SHA-1, SHA-256 and SHA-512
   * Supports RSA-1024, RSA-2048 and RSA-4096

9. Added MTK preloader HASH verification via Android Verified Boot Function

10. Moved Unpack File button to File Tools
   * Unpack Android payload.bin
   * Unpack Oppo OFP Files
   * Unpack Unisoc PAC Files
   * Unpack ASUS RAW Files
   * Unpack Sony SIN Files
   * Unpack Sony FTF Files
   * Unpack LG KDZ Files

11. Improved Android File Tools img2simg (bin to sparse) and simg2img (sparse to bin)

12. Added support for Android Dynamic Fragmented partitions (Read/Write/Erase)
   * These are the partitions normally found inside the super partition for example super___system_a

13. Fixed Samsung Official Firmware Unsparsing Bug 

14. Added Dev Tools tab for Advanced Android OS Tweaking
   * These are only for Developers who know what they are doing
   * Update Hash or HashTree for modified dynamic partitions inside super
   * Re-sign a vbmeta image using a new Private Key in PEM format
   * Example Private Keys in PEM format can be found in 'Android Keys' folder
   * You can also create your own Keys using https://www.cryptool.org/en/cto/openssl/       

15. Added New Samsung eMMC FFU:
   FFU_EMMC_SAMSUNG_WX16MB_KMWX10016M-B619_v0.7.fw (Contributed by kk singh)
  




10.22.2025 - Software and Box Firmware Update

  *** Box Firmware Update is Recommended before using this updated software ***
  
  1. Enabled Scripting support for Custom Made Solutions
     * Big Thanks to the contributors Lemor, MK MOBILE MASTER, Diện Nguyễn and pham ka di.
     * Trainer Scripts updated in the "Scripts" folder
     * User made (3rd Party) scripts can be downloaded through unofficial links 
     * You can Lock and Encrypt a specific Script to work only to a specific F64 Box Serial Number
     * Use 3rd Party Scripts at your own risk

  2. Added Support for SkHynix UFS 2.2 and UFS 2.1 Erase RPMB Data
     * Entire IC will be ERASED including data from ALL LUNs

  3. Added Support for UFS 3.0 Erase RPMB Data when OTP is not Locked 
     * Entire IC will be ERASED including data from ALL LUNs 

  4. Fixed Samsung UFS 2.2 RPMB Data Erase (Thanks to Diện Nguyễn) 

  5. Fixed Factory Provision for Micron UFS 2.2 (Thanks to MSC Solotov)
     * This DOES NOT Erase RPMB Data

  6. Added Support for WriteBooster Automatic Configuration during UFS Provisioning via XML, CSC, PIT and Scatter Files.

  7. Added Support for WriteBooster Automatic Configuration during UFS Provisioning via Mi gpt.img for XRING O1.

  8. Added Support for NEW Exynos Boot Control switch between Slot A to Slot B

  9. Added NEW Exynos Master Boot Record Support for eMMC and UFS

 10. Added NEW Mediatek Master Boot Record Support for eMMC and UFS

 11. Added GPT Support for BMW Automotive. (Thanks, Mr.UPROM!)

 12. Improved Vivo MTK and UniSoc Flashing (Y16, Y21, Y04 etc) (Thanks to hello-firmware.com) 

 13. Improved Itel, Infinix and Tecno MTK and Unisoc Flashing (Thanks to Giovanni Lucas Da Paz)

 14. Enabled dual Slot A and B Flashing for Qualcomm rawprogram.xml files.

 15. Improved Qualcomm Boot Slot change (A/B)

 16. Fixed backup folder name for Samung UFS with a generic "FD10000" serial number
     * Current RPMB Counter will now be appended to the serial number

 17. Added High Light to Secure Write Protected Regions in UFS LUNS (Thanks to Diện Nguyễn)
     * Write Protection can sometimes be removed via ISP multiple Detection 

 18. Added Configuration Lock OTP Status to the main logs for convenience (Thanks to Diện Nguyễn)

 19. Added an option in Settings to "Show Larger UFS Transfer Speed"

 20. EMMC Specifications updated to align with JESD84-B51B (SEPTEMBER 2025)

 21. Added New Samsung eMMC FFU:
     4FEACC : KLM4G1FEAC-C031 (Contributed by 0x9k (Circuit Knight X))
     4FPD3R : KLM4G1FEPD-B031 (Contributed by 0x9k (Circuit Knight X)) 
     4FTE4R : KLM4G1FETE-B041 (Contributed by 0x9k (Circuit Knight X))
     8GME4R : KLM8G1GEME-B041 (Contributed by 0x9k (Circuit Knight X))
     8WMB3R : KLM8G1WEMB-B031 (Contributed by 0x9k (Circuit Knight X))
     AJNB4R : KLMAG1JENB-B041 (Contributed by 0x9k (Circuit Knight X))
     CJNB4R : KLMCG1JENB-B041 v0.6 and v0.7 (Contributed by 0x9k (Circuit Knight X))
     CJTD4R : KLMCG4JETD-B041 v0.4 (Contributed by 0x9k (Circuit Knight X))
     QN16BB : KMQN10006B-B318 (Contributed by 0x9k (Circuit Knight X))
    

 [Improvements of using SoC Firmware 10.20.2025 + ASIC Firmware 10.21.2025]

 22. Targetted IC Detection
     * If the Software is currently in the UFS Tab, the F64 Box will only try to detect using UFS Protocol (Suggested by hello-firmware.com)
     * If the Software is currently in the eMMC Tab, the F64 Box will only try to detect using eMMC Protocol (Suggested by hello-firmware.com)
     * If the Software is NOT in the UFS or eMMC Tab, the F64 Box will try to detect using both UFS and eMMC Protocol

 23. Support for TX_N resistance selection via software control is now available for compatible FPC and ISP Adapters

 24. Enabled Recovery Mode in F64 Box by pressing the Right button then connecting the USB Cable.
     * This will Perform a Factory Reset on the box and can fix common box settings issues such as Boot Loop or strange LCD Colors.


 


09.20.2025 - Internal Exhibition Exe

08.31.2025 - Quick Fix
  1. YMTC EMMC YSxxx Tests

08.28.2025 - Quick Fix

  1. Fixed OEM Unlock bug (Thanks to ABYTECH)

New Samsung eMMC FFU Added:
  QE63MB : KMQE60013M-B318 (Contributed by 0x9k)


08.27.2025 - Update

🚀 Software Update Released: August 26, 2025
We're excited to roll out a major update packed with powerful new features, 
critical fixes, and significant improvements based on community feedback. 
Thank you for your continued support!

F64 Box Firmware & Updates
  Improved F64 Box Firmware Update Process:
    Now supports default Windows Drivers and Android Device Google ADB Drivers.
    Features a simple 1-Click Operation when the F64 Box is in Normal Mode or DFU Mode.

  New F64 Box Firmware (MCU: 08.15.2025):
    Added support for a custom start-up logo.
    Fixed a critical crash issue related to the UART scan.

New RPMB & UFS Features
  Dedicated RPMB Tab: A new, dedicated tab has been added for both eMMC and UFS operations to streamline your workflow.

Universal RPMB Data Erase for UFS:
  *** WARNING: This operation also erases all LUN data. Proceed with caution. ***
  Supports all UFS versions for Samsung brand ICs.
  Supports UFS 3.1, 4.0, and 4.1 for other brands when OTP Configuration is not locked.

SAM RPMB KG Analyzer/Modifier:
  *** You must AGREE to the F64 EULA before using this feature ***
  Added for both eMMC and UFS.
  Note: This feature is for educational purposes only. An RPMB Key is still required to change the KG status.

Automatic Reconnection Loop: Added a new automatic reconnection feature on the UFS tab to improve stability during operations.

General Features & Fixes
  File Loading for RAW Binary Dumps: You can now load files for raw binary dumps, supporting both single RAW images and individual GPT partitions. (Thanks, Mr.UPROM!)
  DDR (RAM Tuning) Erase Button: A new button has been added to erase DDR tuning data, which is useful when changing a device's memory IC. (Thanks, Mr.UPROM!)
  Custom Address Sizing: Added size selection when using custom addressing for RAW reads on both eMMC and UFS.
  Dual FRP Unlock: Added support for unlocking Dual FRP on Samsung devices. (Thanks, Giovanni Lucas Da Paz!)
  Fixed: Corrected an issue with the Dimensity BROM layout header. (A special thank you to Mr. UPROM!)
  Default Setting Change: The "Switch to SLOT A after flashing" option is now UN-CHECKED by default to prevent accidental changes. (Thanks, Mr.UPROM!)
  F64 Box Activation File will now be saved in System Registry as well. (Suggested by Mr 1R0niC);
  F64 Box Calibration File will now be saved in System Registry as well. (Suggested by Mr 1R0niC);

New Samsung eMMC FFU Added:
  3P6CMB : KM3P6001CM-B517 (Contributed by 0x9k)

New Languages Added:
  Marathi, Punjabi, Telugu, Swahili, Hausa, Italian, Polish, Romanian, Japanese and Korean

A huge thank you to our community for the valuable feedback and contributions that 
made this release possible. Your insights help us improve the software for everyone.





07.29.2025 - Update

  1. Improved FRP Handling for phones that transitioned from Android 14 to Android 15 (Thanks to Giovanni Lucas Da Paz)

  2. Added Automatic FRP Disable in Settings -> Advanced Tasks Tab (Requested by Lemor PH)

  3. Now shows FRP Status (Active / Not Active) if FRP is used by the phone (Requested by KUMAR ALOK VISHWAKARMA)

  4. Added support for RAW Binary Image file dumps from other Tools. (Requested by Mr.UPROM)
     * As of now, only GUID Partition Table is supported. More partition formats will be added soon.
     * PrimaryGPT can be selected or unselected
     * All Partitions inside the RAW Binary Image dump can be selected or unselected 

  5. Added Android Slot A/B Change for Qualcomm SoC-based Phones (Requested by hello-firmware.com) 

  6. Added GPT Master Tools (GUID Partition Table) (Requested by 元亿科技)
     These features are accessible by right-clicking any partition in Partitiion Table List

     * Resize any existing Partition (Change First LBA or Last LBA)
     * Rename Partition
     * Change GUIDs 
     * Change Flags (Priority, Tries Left, Successful, Read Only etc...) 
     * Manual GUID Input and Random GUID Generation Supported 
     * Delete Partitions
     * Create New Partitions using Free Space markers (free_space_X)
     
  7. Added Android File Tools (Requested by hello-firmware.com)      

     * Convert Binary Dump into Android Sparse File img  (img2simg)
     * Convert Single Sparse File into Binary Dump (simg2img)
     * Convert Multiple Sparsed Files into 1 Binary Dump
         example: super.img_sparsechunk.0
                  super.img_sparsechunk.1
                  ....
                  super.img_sparsechunk.21
     * Optional Data Trim for trailing blank space
    
  8. Added Automatic Box Firmware Download from server via "Write Box Firmware" or Box Firmware Update
     * DFU and Normal Mode supported
     * Just make sure DFU Mode is not using Android Device drivers.
       Uninstall + Delete Android Device Drivers if necessary

  9. Now you can use a Custom CompanyLogo.bmp for the User Interface

     * Bitmap Files with 500 x 500 pixels are supported
     * Replace the file 'Image\CompanyLogo.bmp' with your Personal Logo

 10. Fixed Android Sparse File Bug on Moto Firmware (Thanks to Master Unlock GSM). 

 11. Added Boot Partition display in Logs for UFS (Thanks to KUMAR ALOK VISHWAKARMA)

 12. Fixed preloader Boot Relay Table for Vivo Y02T and Y21 (Thanks to hello-firmware.com)
 
 13. Added "Do not Write to Disk" option in Software Settings
     * This can be used to read the entire IC memory without saving it to your PC Storage
     * This is useful if you want to perform a complete IC Read Memory Test

 14. Added Android Slot Write Option after Firmware Flashing
 
 15. Initial HiSilicon eMMC Partition Support for Android TV (Romeo Tabios)
     * Full Read Android Information Reading for non-encrypted Devices

 16. Initial U-BOOT eMMC Partition Support for Android TV (Thanks to Nghĩa Trần Đình)
     * Partition Information Only
     * Android/Linux Information not yet available 

 17. Added New Samsung eMMC FFU:
     FNX2MB : KMFNX00012M-B214  
     8GTF4R : KLM8G1GETF-B041 (by Diện Nguyễn)
     RH64AB : KMRH60014A-B614 (by Ahmed El-Zawawy)
     3V6CBB : KM3V6001CB-B708 (by Ahmed El-Zawawy)

 18. Added new Software GUI Language Packs (Machine Translated):
     *** Warning : These are machine translated by Gemini 2.5 Pro and may contain errors in translation ***
     Arabic, Bengali, French, German, Hindi, Indonesian, Portuguese, 
     Russian, Malay, Turkish, Ukrainian, Urdu, Vietnamese



07.04.2025 - Server Update

  1. Updated Server Authentication

  Important Notice: Software Compatibility Update

  Older versions of the F64 Software will no longer be 
  able to connect to the server.

  If you are registering a new box, please download and 
  use the latest software version available from our official 
  website: www.flash64.com.

  Older software versions will continue to work with new boxes 
  as long as the box firmware version is supported.

  To continue using an older version of the F64 Software, 
  you can copy the Activation folder from the newer version's 
  directory and paste it into the older version’s folder.
   

  2. Format Partition as EXT4 added for both eMMC and UFS

  3. Format Partition as F2FS added for both eMMC and UFS

  4. Initial Amlogic eMMC Partition Support for Android TV (Thanks to Diện Nguyễn & Romeo Tabios)
     * Full Read Android Information Reading for non Encrypted Devices
     * eMMC Resize via MBR button

  5. Initial MStar eMMC Partition Support for Android TV (Thanks to Diện Nguyễn & Romeo Tabios)
     * Full Read Android Information Reading for non Encrypted Devices
     * eMMC Resize via MBR button

  6. Initial LG Web OS eMMC Partition Support for Android TV (Thanks to Diện Nguyễn)
     * Full Partition Info Reading
     * eMMC Resize via MBR button

  7. Fix GUI hang during Micron eMMC FFU

  8. Fixed IMEI Detection on Samsung Exynos


06.16.2025 - Update

  1. Added Support for adding Custom Watermark to Software GUI

  2. Added Option to use Calibration Trim for a more accurate VCCQ setting

  3. Added Support for Samsung sec_efs information parsing (IMEI*, SN* etc) *if available

  4. Added Support for Unisoc UFS Devices Flashing using Official Firmware

  5. Added Support for Motorola Unisoc UFS/eMMC Flashing via .bat files Official Firmware (Thanks to Giovanni Lucas Da Paz)

  6. Improved eMMC Android Sparse Flashing (Thanks to KUMAR ALOK)

  7. Improved UFS Android Sparse Flashing

  8. Fix MBR Repair button for eMMC (Thanks to KUMAR ALOK)

  9. Fix GPT Generate button for eMMC (Thanks to KUMAR ALOK)

 10. Added SKU to Phone Model matching for Infinix

 11. Added support for reading Android Information on Exynos 1580 phones (Thanks to Efrén Hernández)

 12. eMMC and UFS Health report will now be shown in Bright RED if 80% or above (Thanks to KUMAR ALOK)

 13. Fixed eMMC RAW Write for BOOT A and BOOT B (Thanks to hello-firmware.com)
 
 14. Added Samsung FFU Erase Option

 15. Added New Samsung eMMC FFU:
     3P6CMB : KM3P6001CM-B517 (by ratna mobiles Tamilnadu)
     MAG2GC : KLMAG2GEAC-B001 (by FarshiD)
     Q313MB : KMQ310013M-B419 (by FarshiD)
     4X6KMB : KM4X6001KM-B321 v0.9 (by hello-firmware.com)

 16. Added New Micron eMMC FFU:
     MICRON_G1C155
     MICRON_G1C156
     MICRON_G1J38E
     MICRON_G1J39E
     MICRON_G1J9P8
     MICRON_G1J9Q9
     MICRON_G1J9R8
     MICRON_G1J9S9
     MICRON_G2C213
     MICRON_G2C214
     MICRON_G2C215
     MICRON_G2C218
     MICRON_G2C219
     MICRON_G2M211
     MICRON_G2M212
     MICRON_S0J97Y
     MICRON_S0J9D8
     MICRON_S0J9K9
     MICRON_S0J9N8


06.02.2025 - Update
  
  1. Added Support for Xioami Xring O1 Devices (Xiaomi 15S Pro, Xioami Pad 7 Ulta, etc)
     * UFS Provisioning supported via gpt.img (Xioami GPT File)
     * Full Firmware Flashing supported via flash.bat / flash.sh
     * Full Firmware Flashing supported via fdt_sec.xml (Xioami XML File)   

  2. Added Support for SPD/Unisoc FileList.ini Flashing using Official Firmware

  3. Added Motorola UTAG partition parsing (Thanks to Mr.UPROM)

  4. Added SKU to Phone Model matching for Samsung, Vivo, Realme, Oppo, Nubia and Xiaomi_models

  5. Added skip Userdata option for RAW Partition Reading (Thanks to Mr.UPROM)

  6. Added quick access to eMMC Boot Configuration in Partition Tab (Thanks to yu luosheng)

  7. Fixed Exynos impoper parsing of partitions inside SUPER (Thanks to Giovanni Lucas Da Paz)

  8. Improved "AI Connect" for eMMC ISP Flashing Sparsed Files (Thanks to hello-firmware.com)

  9. Improved eMMC Erase Function

 10. Improved COMBO_BOOT detection on MTK Preloaders (Thanks to hello-firmware.com)

 11. Added New Samsung FFU:
     GP6BAB : KMGP6001BA-B514 (by 0x9k)
     CUTB42 : KLMCG2UCTB-B041 (by hello-firmware.com)
     GX6BMB : KMGX6001BM-B514
     RD64MB : KMRD60014M-B512
     RH64AB : KMRH60014A-B614
     RE1BMB : KMRE1000BM-B512
     RC1BMB : KMRC1000BM-B809
     FE12MB : KMFE10012M-B214
     BWBD3R : KLMBG4WEBD-B031


05.19.2025 - Update

  1. Fixed a MAJOR erase bug on small eMMC partitions (Thanks to hello-firmware.com).

  2. Added MTK Direct Preloader Header Generation for manually loaded files (Thanks to hello-firmware.com).

  3. Improved Android Security automatic backup file saving (Thanks to Giovanni Lucas Da Paz).

  4. Improved rawprogram.xml universal backup file format (Thanks to Master Unlock GSM).

  5. Moved BOOT A and BOOT B eMMC partitions to the top (Thanks to sohrab ezi).

  6. Fixed BOOT A and BOOT B raw partition writing (Thanks to sohrab ezi).

  7. Fixed Unisoc SPL loader flashing for Samsung factory files (Thanks to Nguyễn Diện and Giovanni Lucas Da Paz).

  8. Added "Backup Security" button** in the Partitions tab.

  9. Moved "Erase Before Write" option in the Partitions tab.

 10. Added "Fake" Health Repair firmwares for SK Hynix hB8aP>, hC8aP>, hC9aP3, and hDEaP3

    * These FFU firmwares do not repair health, but only make the eMMC report that its health is "Perfect."
    * These FFU firmwares have "\_HR" at the end of the filename, e.g., 30_HYNIX_hB8aP__0060_PATCHED_FINAL_HR.fw.
 
 11. Samsung eMMC FFU Filename now includes the IC Marking (Thanks to sohrab ezi).

 12. Added New Samsung FFU:
     QE13MB : KMQE10013M-B318 (by 0x9k)
     QX63AB : KMQX60013A-B419 (by 0x9k)
     MCG8GC : KLMCG8GEAC-B001
     DH6DMB : KMDH6001DM-B422
     RX14MB : KMRX10014M-B614
     QX13MB : KMQX10013M-B419
     RX1BMB : KMRX1000BM-B614
     RX64MB : KMRX60014M-B614

 13. Improved MTK Preloader IC Check for supported UFS / EMMC check

 14. Added MBR/GPT repartition support for Phones that does not use BackupGPT (Kirin based) (Thanks to Mr.UPROM).

 15. Fixed UFS Provisioning of LU Dedicated WriteBooster (Thanks to Giovanni Lucas Da Paz). 

 
04.30.2025 - Update

  1. Fixed Android Info Reading for Motorola Phones

  2. Fixed Boot Mode eMMC FFU to not change CID

  3. Fixed Micron UFS Provision Bug

  4. Added UFS Erase all LUNS Button
     * Use this to fix "slow" UFS IC
     * This is a safer option than Provisioning the UFS
     * Does not require OTP Unlock
     * Does not Erase RPMB Data
     * Does not Erase Write Protected Areas

  5. Added eMMC Erase All Partitions Button
     * Use this to Erase all Data from the eMMC
     * Resets eMMC BOOT Config
     * Does not Erase RPMB Data 

  6. Added Samsung eMMC Firmwares
     DUTB42 : KLMDG4UCTB-B041
     3H6CAB : KM3H6001CA-B515 
     DP68MB : KMDP60018M-B425 (by 0x9k)
     DV6DAB : KMDV6001DA-B620 (by 0x9k)

  7. Added Generic Android OEM Unlock
     * Additional Steps may be required to
       fully unlock the bootloader of the phone
       depending on the phone brand/manufacturer
 
  8. Added RPMB Write for UFS

  9. Improved Read/Backup Partition file (rawprogram.xml)
  
 10. Added EXT_CSD as part of eMMC Partition List

 11. Added Primary GPT and Backup GPT Check upon IC Detection (Thanks to KHUMAR ALOK VISHWAKARMA)

 12. Improved GPT Generation for Dimensity and Qualcomm UFS and eMMC (Thanks to Mr.)

 13. Automatic Boot Slot Selection when using flash_all.bat mi Factory Firmwares   

 14. Added Adjustable EMMC VCC On delay via Settings.ini EmmcVccInitDelay=2000 Entry
     * This value is in milliseconds
     * Adjustable from 40 upto 8000 milliseconds


03.29.2025 - Update

  1. Fixed Vivo Red State after FRP.
     
     *** Always Select "FRP New Security (2024, 2025) for newer Android 14 and 15 phones

  2. Added a more visible Location for the following information:
       Boot Partition
       Reference Clock
       Configuration Descriptor (OTP)
       Partition Setting Locked (eMMC)
 
  3. Added dLUNumWriteBoosterBufferAllocUnits in saving and writing UFS provision.xml
 
  4. Improved eMMC ISP Read Speed

  5. Improved Samsung FRP Remove


03.21.2025d - Quick Fix
   
  1. Fixed eMMC Qualcomm GPT file loading. (Thanks to SadaM)

03.21.2025 - New Features and Bug Fixes

  1. Added eMMC RPMB Set Counter to match previous RPMB Counter on Qualcomm Phones (Requested by Ramana)

  2. Fixed Samsung eMMC RPMB Size Change (Reported by Abdullah Rasheed)

  3. Fixed eMMC RPMB Read Counter Stuck on ISP

  4. Added automatic loading of Qualcomm gpt_main0.bin, gpt_main1.bin etc in partition list.
     * With automatic Repartition.

  5. Added Android Boot slot Change A/B 

  6. Remove Factory Reset Button in Partition List
     * Now you need to use Erase User Data and choose the proper option best suited for
       your phone. Do this AT YOUR OWN RISK.
 
  7. Added Samsung eMMC Firmwares
     CKTA42 : KLMCG2KCTA-B041
     CUTA42 : KLMCG2UCTA-B041
     DD68MB : KMDD60018M-B320
     DH6DAB : KMDH6001DA-B425
     DP6DBB : KMDP6001DB-B425
     DUTA42 : KLMDG4UCTA-B041
     DV6DBB : KMDV6001DB-B620
     DV6DMB : KMDV6001DM-B620
     DX68MB : KMDX60018M-B425
     FE62MB : KMFE60012M-B214
     GP6BMB : KMGP6001BM-B514
     GX6BAB : KMGX6001BA-B514
     QX63AB : KMQX60013A-B419
     QX63MB : KMQX60013M-B419

  8. Added SkHynix eMMC Fimrwares
     H8G4a2
     HAG4a2
     HCG8a4

  9. Fixed SGPT Generation for MTK and Qualcomm


02.27.2025 - End User Requests and Bug Fixes

  1. Added AI Connect (Autonomous Interaction)
     This feature will automatically reconnect if communication 
     errors are detected. This helps when connecting phones
     via ISP using USB power only (No Vcc and VccQ). The feature
     is enabled by default.

  2. Added support for malformed GPT Headers from some Moto Phones.

  3. Added EMMC Firmware Contributed by End User
     QE63MB : KMQE60013M-B318 (by s.l.m.)


02.24.2025 - End User Requests and Bug Fixes
  
  1. Fixed Erase of very small partition sizes

  2. Remove nag Screen "Please click Yes 3 times"

  3. Increased UFS Inactivity Timeout 


02.23.2025 - End User Requests and Bug Fixes
  
  1. Fixed GPT and SGPT Sizes for newer MTK based Soc

  2. Fixed FRP on older Androids - Thanks to KUMAR VISHWAKARMA

  3. Added EMMC Firmware Contributed by End User
     3V6CAB : KM3V6001CM-B708 (by Bilal Akash)


02.18.2025 - End User Requests and Bug Fixes

  1. Added New FRP Remove Option for persistent partition data fill
     * You can now select to fill partition with 0xFF or 0x00
  
  2. Added EMMC Firmware Contributed by End Users:
     3V6CBB : KM3V6001CM-B705 (by yu luosheng)

  3. UFS Amplitude Setting now defaults at 316 mV for more compatibility


02.15.2025 - End User Requests and Bug Fixes

  1. Initial support for Monitors with less than 1080p Resolution

  2. Added EMMC Firmware Contributed by End Users:
     RC14MB : KMRC10014M-B809 (by SadaM)
     BJTD4R : KLMBG2JETD-B041 (by SadaM)
     GX6BAB : KMGX6001BA-B514 (by SadaM)
     DV6DBB : KMDV6001DB-B625 (by SadaM)
     QD63MB : KMQD60013M-B318 (by SadaM)
     QX63AB : KMQX60013A-B419 (by SadaM)


02.14.2025 - End User Requests and Bug Fixes
  
  1. Fixed sboot target partition from PIT for the following Exynos SoC:
    * Reported by MasterUnlockGSM from Venezuela    
       Exynos 1280
       Exynos 1330
       Exynos 1380
       Exynos 1480
       Exynos 1580
       Exynos 2200
       Exynos 2400
    
    
  2. Added PIT File Support for UFS Provisioning

  3. Fixed MTK Preloader Boot Relay Table for newer SoCs (UFS and EMMC)     
    * Reported by Knotthailand

  4. Added SkHynix EMMC FFU files for:
       hB8aP>
       hC8aP>
       hC9aP3
       hDEaP3

    * These eMMC Firmware will allow RPMB Key Reading, Unlimited Repartitioning, WP Removal and CID/CSD Write
    * Performing FFU on SK Hynix eMMC will NOT result in data loss.
    * Avoid performing multiple FFU operations on the same eMMC, as its firmware uses a static NAND page address. 
      This means the page cannot be relocated if bad blocks begin to develop.

  5. Added the ability to set the working directory using the HOME button located at the lower right corner of the software.
     * Suggested by MasterUnlockGSM from Venezuela

  6. A separate rawprogram.xml per LUN will now be generated during partition backups.
     * Suggested by MasterUnlockGSM from Venezuela

  7. Enhanced the speed of FFU reading for Samsung eMMC.

  8. UFS VCC is now set to 2.80V by default.

  9. Added support for UFS 4.1 new descriptors, attributes and flags.


02.05.2025 - End User Requests and Bug Fixes

  1. Added eMMC Boot Config Information in Connection Logs

  2. Added Auto LBA Skip on eMMC with Secure Write Protected Blocks

  3. Added Detailed Connection ERROR Resolution for UFS ISP

  4. Added EMMC Firmware Contributed by End Users:
     DV6DAB : KMDV6001DA-B620 (By Knotthailand)
     GD6BMB : KMGD6001BM-B421 (By Knotthailand)
     DC6DMB : KMDC6001DM-B625 (By Knotthailand)

  5. Fixed GUI Freeze on UFS and EMMC Read Timeouts


02.01.2025 - Initial Update and Bug Fixes
  
  1. Added Auto LBA Skip on UFS with Secure Write Protected Blocks

  2. Added UFS Secure Write Protection Removal (WP Remove)

     ** Use this option at your own risk **

     According to our tests, most UFS will suffer 100% Data Loss with
     a very few exception listed below
     
     Brand  | UFS Specification | Data Status after WP Remove
    -------------------------------------------------------------
    Samsung | 2.0               | NO Data Loss
    Samsung | 2.1               | NO Data Loss
    Samsung | 2.2               | NO Data Loss
    Samsung | 3.0               | NO Data Loss
    Samsung | 3.1               | NO Data Loss
    Samsung | 4.0               | WARNING 100% Data Loss on all LUNs !!! - make backup all LUNs !!!
    -------------------------------------------------------------
    YMTC    | 2.2               | NO Data Loss
    -------------------------------------------------------------
    Other Brands (SkHynix, Micron, KIOXIA etc...) will experience 100% Data Loss on all LUNs !!! - make backup all LUNs !!!


01.22.2025 - Initial Early Release







Official Releases

  NONE
     


             