Establish Connection
Take Screenshot
Clear Logs
Stop Task
Address
Size
Transfer Speed
Estimated Time Left
Show Box Wallpaper
Device Information
Connect
MAIN
Partitions
Flash Memory Information
Product Name
Manufacturer ID
Total Raw Device Capacity
Number of Logical Units
Specification Version
Manufacturing Date
LUN
Partition Name
Filename
Block Address
Size
Type
Status
Android Partition Tasks
Read
Write
Erase
Graph
Space Allocation
UFS
Connection Parameters
Warning: UFS 4.x can be damaged above VCC 2.90
Signal Booster (ISP)
This is for UFS 4.x HS-LSS only
B-series is slightly faster than A-series
RAW Access
Read
Write
Erase
Logical Unit
Size
Write Padding Byte
Erase Options
Erase Single LUN
Wipe Entire Device
Custom Address
Start Address
End Address
Address Type
Sector
Byte
SCSI Options
Descriptors
Device
Configuration
Size
Unit
Interconnect
String
Geometry
Power
Health
FBO
FBO Specification Version
Recommended LBA Range Size
Maximum LBA Range Size
Minimum LBA Range Size
Maximum Number of LBA Ranges
Alignment Requirement
Attributes
Flags
eMMC
Connection Parameters
For ISP, use slow CLOCK (6.5 Mhz  etc.)
Connect
Stop
RAW Access
Read
Write
Erase
Partition
Size
Erase Options
Erase
Discard
Secure Erase
Trim
Secure Trim
Sanitize (Secure Data Removal)
Custom Address
Start
End
Address Type
Sector
Byte
Write Padding
Byte
Skip Firmware Erase
Connection Tasks
Check eMMC Status
Check eMMC Health Report
RPMB Options
Counter
Secure Write Protect Configuration
Secure Write Protect Enable
Use RPMB Key
Generate Random Key
Write RPMB Key
Read RPMB Key
Test RPMB Key
Partitions
Write to eMMC
Reset Changes
Save to File
Open File
Enhanced Area Start
Health Check
Vendor Health Report
Provisioning
Hardware
Box Appearance
LCD Theme
LCD Brightness
RGB Brightness
RGB Theme
Read Settings
Save Settings
Color Picker
Boot Logo
Change Wallpaper
Box Features
Calibrate Voltage
Memory Info
Restart USB
Write Box Firmware
Active Buzzer Notifications
Simulation Mode
Calibration Trim
Box Information
Box Type
F64 Serial Number
Bluetooth LE MAC Address
Activation File Version
Support Link
Software
Partition Table Font Size
Software Log Font Size
Enable Sound Effects
Show Hints
Prioritize UFS 4.x Detection
Show Progressbar Percentage
Show Partition List Grid
Do not Write to Disk (For Memory Test Only)
Show Speed Gauge
Read Android Information
Android Security Partition Backup
Show UFS Debug Connection
Android Partition Analyzer
Read RPMB Information
Slow Read/Write (For Bad eMMC IC)
UFS Read S.M.A.R.T. Report
Connect BLE
Visual Themes
Skin Theme
JEDEC Logs Text Color
Set color
WriteBooster Buffer configuration:
Verifying Secure Bootloader...
Device type:
UFS Device Class:
UFS Mass Storage Subclass:
Protocol supported by UFS Device:
Boot Enable:
Short Boot Enable:
Boot Sequence ID:
Support for security LU:
Specification version:
Manufacturing Date:
Number of Well known Logical Units:
Descriptor Access Enable in Partial Initialization:
Initial Power Mode:
High Priority LUN:
Secure Removal Type:
Background Operations Termination Latency:
Initial Active ICC Level:
Unit Descriptor 0 Base Offset:
Unit Descr. Config. Param. Length:
RTT Capability of UFS Device:
RTC Update:
UFS Features Support:
Field Firmware Update Timeout:
Queue Depth:
Device Version:
Number of Secure Write Protect Areas:
PSA Maximum Data Size:
PSA State Timeout:
WriteBooster uses User Space:
WriteBooster Buffer Type:
WriteBooster Buffer size for the shared
UM CPort Configuration:
Unified Memory Minimum Area Size
HPB Specification Version:
HPB Control Mode:
Number of Logical Units:
Boot Config Length:
Logical Unit Configuration Length:
RPMB Region Enable:
RPMB Region 1 Size:
RPMB Region 2 Size:
RPMB Region 3 Size:
Logical Unit Enable:
Boot LUN ID:
Logical Unit Write Protect:
Memory Type:
Number of Allocation Units:
Data Reliability:
Logical Block Size:
Provisioning Type:
Context Capabilities:
WriteBooster Buffer Size:
HPB Maximum Regions:
HPB Pinned Region Start Offset:
HPB Pinned Regions:
Unit Index:
Logical Unit Queue Depth:
Logical Unit Queue Priority:
Data Type Support:
Logcial Block Count:
Erase Block Size:
Production State Awareness Sensitivity:
RPMB Region 0 Size:
Physical Memory Resource Count:
Granularity of the Large Unit:
Maximum Number of Active HPB Regions:
Number of HPB Pinned Regions:
Logical Unit WriteBooster Buffer Size:
MIPI Unipro Release Version Number:
MIPI M-PHY Release Version Number:
Manufacturer Name:
Product Name:
OEM ID:
Serial Number:
Product Revision Level:
Total Sector Count:
Native Block Size:
Segment Size:
Allocation Unit Size:
Minimum Addressable Block Size:
Optimal Read Block Size:
Optimal Write Block Size:
Maximum Data-in Buffer Size:
Maximum Data-out Buffer Size:
Maximum Data Size in a Phase Collapse:
Support for Out-of-Order Data Transfer:
Maximum Number of Logical Units Supported:
Maximum Number of RPMB Frames:
Dynamic Capacity Resource Policy:
Maximum Available Contexts Supported:
System Data Tag Unit Size:
System Data Tag Resource Size:
Supported Secure Removal Types:
Supported Memory Types:
Number of Memory Types Supported:
Enhanced Memory Type 1:
Enhanced Memory Type 1 Maximum Allocation Units:
Enhanced Memory Type 1 Capacity Adjustment Factor:
System Code Memory Max Allocation Units:
System Code Memory Capacity Adjustment Factor:
Non-Persistent Memory Maxi Allocation Units:
Non-Persistent Memory Capacity Adjustment Factor:
Enhanced Memory Type 1 Max Allocation Units:
Enhanced Memory Type 2 Max Allocation Units:
Enhanced Memory Type 2 Capacity Adjustment Factor:
Enhanced Memory Type 3 Max Allocation Units:
Enhanced Memory Type 3 Capacity Adjustment Factor:
Enhanced Memory Type 4 Max Allocation Units:
Enhanced Memory Type 4 Capacity Adjustment Factor:
Optimal Logical Block Size:
UFS Device Maximum WriteBooster Buffer Size:
UFS Device Maximum WriteBooster Buffer Count:
WriteBooster Capacity Adjustment Factor:
WriteBooster User Space Consumption Mode:
Maximum Zoned logical units:
Zoned logical unit Minimum Erase Bytes:
Zoned logical unit Size:
HPB Region Size:
HPB Maximum number of LU:
HPB Sub-Region Size:
HPB Maximum Active Regions:
Maximum VCC Current:
Maximum VCCQ Current:
Maximum VCCQ2 Current:
Pre End of Life Information:
Life Time via Vendor Method A:
Life Time via Vendor Method B:
Total Refresh Count:
Refresh Progress:
Vendor Proprietary Health Report:
Device Initialization:
Permanent Write Protection:
Power On Write Protection:
Background Operations:
Purge Operation:
Purge Error Status:
Out of Order Data Feature:
Device Life Span Mode:
Purge Enable:
Refresh Enable:
Physical Resource Removal:
Real Time Clock:
UM Initialization:
Field Firmware Update Operation:
UM Suspend Command:
UM Suspend Status:
WriteBooster Feature:
WriteBooster Flush Operation:
WriteBooster Flush During Hibernate:
Host Performace Booster Reset:
Host Performance Booster Enable:
Boot LUN:
Current Power Mode:
Active ICC Level:
Power On Reset Device State:
Background Operation Status:
Purge Operation Status:
Maximum Data In Size:
Maximum Data Out Size:
Out of Order Data Transfer Feature:
Dynamic Capacity Needed:
Reference Clock Frequency Value:
Configuration Descriptor Lock:
Exception Event Control:
Exception Event Status:
Unified Memory Area Size:
UM Max UMPIU Requests:
Maximum HPB Command Data Size:
Seconds Passed from TIME BASELINE:
Context Configuration:
Correctly Programmed Blocks:
Device FFU Status:
Production State Awareness Status:
Production State Awareness Data Size:
Reference Clock Gating Wait Time:
Rough Package Case Surface Temperature:
High Temperature Boundary:
Low Temperature Boundary:
Throttling Status:
WriteBooster Buffer Flush Status:
Available WriteBooster Buffer Size:
WriteBooster Buffer Life Time:
Current WriteBooster Buffer Size:
EXT_IID Status:
Host Hint Cache Size:
Refresh Operation Status:
Refresh Frequency:
Refresh Operation Unit:
Refresh Method:
Timestamp Since January 1, 1970 (UTC):
FBO Operation Control:
FBO Optimization Level:
FBO Current State:
F64 Serial Number: 
Bluetooth LE MAC Address: 
Box Type: 
Debug Level: 
Activation File Version: 
Timestamp: 
Connect
Click this
Disconnect
Hide Box Wallpaper
Show Box Wallpaper
BLE Connected
Wrong PIN
SD Card
eMMC
UFS
Searching Devices...
Write to eMMC
Partitions Already Configured
Read / Set only
Read / Write once
Read / Power on reset
Read / Volatile
Write only / Volatile
Read
Read / Persistent
Read only
Clear
Set
Language
Tools
Tools
Diagnostic Tools
General Settings
Online Support
Full User Area Logical Erase
Connection Tasks
Boot Partition
User Area Partition
General Purpose Partition
Text Copied
Next Page
Previous Page
Amplitude Adjust
Enable 
Signal Amplitude
Invert
Use this for
Use only for
Memory Access
Slave Address
Register
Detected Slaves
Swap SDATA and SCLK
Power Down VIO after Scanning
Swap SDA and SCL
Power Down VDD after Scanning
Start Scanning
Show Pinout
Selected value will make

Are you sure you want to continue?
Value Needed
Please Enter a Hexadecimal Value
click here to write value
FBO Specification Version:
Recommended LBA Range Size:
Maximum LBA Range Size:
Minimum LBA Range Size:
Maximum Number of LBA Ranges:
Alignment Requirement:
click here to change value
click here to read value
Click here to safely Power Down the IC
The device has entered UFS-PowerDown Mode
The device has entered EMMC_POWER_OFF Mode
You can now safely remove it from the Socket
Test RPMB Write
Purge RPMB
RPMB Options
Entry
Secure Write Protect Configuration
Logical Block Address
Number of Logical Blocks
Write Protection Type
Boot Configuration
Boot Partition
Boot Bus Width
Boot Mode
Boot Acknowledge
Reset bus width after Boot
Permanent Boot Configuration Protection
Write Protection Configuration
Boot Area 1 WP Status
Boot Area 2 WP Status
Temporary Write Protection
Permanent Write Protection
Secure WP Support
Secure WP Status
Fast RPMB Read
Write Reliability Settings
Reset RPMB
Advanced Tasks
Reset Counter
Unlock CSD
Full Factory Reset
Reset Signal
Dynamic Capacity Management
Secure Bad Block Management
Dynamic Capacity Needed Status
Factory Reset
Custom WP Area
Manage Dynamic Capacity
Scan eMMC WP-Groups
Remove Write Protection
Automatic Reconnection Loop
Adjusts Differential Voltage Swing
Read S.M.A.R.T. Information
Write Protection Information
B_PWR_WP_EN
Unchecked: Boot region is not power-on write protected.
Checked: Enable Power-On Period write protection to the boot area. This bit must be zero if B_PWR_WP_DIS (bit 6) is set. When read, this bit only indicates if power-on protection has been set specifically for a boot region. How power-on protection has been applied depends on the setting of bits 7 and 1. To verify boot region protection read BOOT_WP_STATUS[174].
B_PWR_WP_SEC_SEL
Unchecked: B_PWR_WP_EN (bit 0) applies to boot area only, if B_SEC_WP_SEL (bit 7) is set.
Checked: B_PWR_WP_EN (bit 0) applies to boot area only, if B_SEC_WP_SEL (bit 7) is set.
B_PERM_WP_EN
Unchecked: Boot region is not permanently write protected.
Checked: Boot region is permanently write protected. This bit must be zero if B_PERM_WP_DIS is set. When read, this bit only indicates if permanent protection has been set specifically for a boot region. How permanent protection has been applied depends on the setting of bits 7 and 3. To verify boot region protection read BOOT_WP_STATUS[174]. This bit may be zero if the whole device is permanently protected using CSD[13].
B_PERM_WP_SEC_SEL
Unchecked: B_PERM_WP_EN (bit 2) applies to boot area only, if B_SEC_WP_SEL (bit 7) is set.
Checked: B_PERM_WP_EN (bit 2) applies to boot area only, if B_SEC_WP_SEL (bit 7) is set.
B_PERM_WP_DIS
Unchecked: Master is permitted to set B_PERM_WP_EN (bit 2).
Checked: Permanently disable the use of B_PERM_WP_EN (bit 2). This bit must be zero if B_PERM_WP_EN is set. This bit has no impact on the setting of CSD[13].
B_PWR_WP_DIS
Unchecked: Master is permitted to set B_PWR_WP_EN (bit 0).
Checked: Disable the use of B_PWR_WP_EN (bit 0). This bit must be zero if PWR_WP_EN is set.
B_SEC_WP_SEL
Unchecked: B_PERM_WP_EN (bit 2) and B_PWR_WP_EN (bit 0) apply to both boot partitions and B_PERM_WP_SEC_SEL (bit 3) and B_PWR_WP_SEC_SEL (bit 1) have no impact.
Checked: B_PERM_WP_EN (bit 2) and B_PWR_WP_EN (bit 0) apply to only the boot partition selected by B_PERM_WP_SEC_SEL (bit 3) and B_PWR_WP_SEC_SEL (bit 1) respectively.
NOTE: Once a device has been set to enable protection on the boot partitions separately, this cannot be reverted for a power cycle. This bit enables a mix of permanently protected and power-on protected boot partitions.
US_PWR_WP_EN
Unchecked: Power-on write protection is not applied when CMD28 is issued.
Checked: Apply Power-On Period protection to the protection group indicated by CMD28. This bit cannot be set if US_PWR_WP_DIS is set. This bit has no impact if US_PERM_WP_EN is set.
US_PERM_WP_EN
Unchecked: Permanent write protection is not applied when CMD28 is issued.
Checked: Apply permanent write protection to the protection group indicated by CMD28. This bit cannot be set if US_PERM_WP_DIS is set.
US_PWR_WP_DIS
Unchecked: Power-on write protection can be applied to write protection groups.
Checked: Disable the use of power-on period write protection for write protection groups within all the partitions in the user area from the point this bit is set until power is removed or a hardware reset occurs. Setting this bit does not impact areas that are already protected.
US_PERM_WP_DIS
Unchecked: Permanent write protection can be applied to write protection groups.
Checked: Permanently disable the use of permanent write protection for write protection groups within all the partitions in the user area from the point this bit is set forward. Setting this bit does not impact areas that are already protected.
CD_PERM_WP_DIS
Unchecked: Host is permitted to set PERM_WRITE_PROTECT (CSD[13]).
Checked: Disable the use of PERM_WRITE_PROTECT (CSD[13]).
PERM_PSWD_DIS
Unchecked: Password protection features are enabled.
Checked: Password protection features (ERASE (Forcing erase), LOCK, UNLOCK, CLR_PWD, SET_PWD) are disabled permanently.
Use
to modify PERM_WRITE_PROTECT and TMP_WRITE_PROTECT values
Format as exFAT
Overwrite Existing File?
Operation Cancelled...
Save RAW Flash Dump File
Select Output Directory
Save RAW Register Dump File
Open a BitMap File
Select Flash File
Write RAW Flash Dump File
Write EXT_CSD File
Select Binary FFU File
Repair
Full Factory Reset eMMC?
Continue anyway?
This will erase DATA, BOOT, RPMB and all other Settings.
Are you sure you want to Erase?
Are you sure you want to Write?
Erase Partition before Write?
Read super Partition Information
Write Userdata?
Are you sure you want to Erase
Do you want to Format
Are you sure you want to Erase Entire Device?
Unlock/Reset CSD?
Not all eMMC / eMCP Supports this feature.
Remove USER Area and GPPx Write Protections?
Write CID Register?
Write Secure WP Configuration?
A successful write will add 2 to the RPMB Counter.
ARE  YOU  SURE ???
Write RPMB Key?
A successful write will add 1 to the RPMB Counter.
Test RPMB Write?
Load XML for other Partitions?
Search...
Search Partition
Search Next
Load Older Backup
No More Older Backups Found!
Load Newer Backup
No More Newer Backups Found!
Configuration Loaded from
Time Stamp
Configure
Repair GPT Errors if found? 
Unpack Files
Select Packed Files
Verify Checksums and Hash?
Select Country / Provider Variant Code
FRP Unlock
Format FRP Partition?
Erase User Data
Erase User Data?
Are you 100% Sure?
User Data will be lost forever.
Are you sure you want to continue?
Factory Format Device?
Factory Format Device
Blank Check
Decompressing File
Please wait...
Reading Android Information
I understand that I can only use these features for
experimental purposes on devices that I own.

Account Remove
Do you confirm that this is your device?
Unpacking File
Verifying Checksum
Click the Write button to apply UFS Provisioning
Factory Provision
Warning:
Changes in UFS Provision settings will ERASE ALL DATA inside the UFS ic.
Make sure you have made a backup of all important partitions before proceeding.
Current UFS Provision saved to:
Applying Persistent Attributes:
Register F64 Box
Please input all required information
is Required
not the same as
First Name
Last Name
Email Address
Country
Mobile Number
Message Service
User Name
OTP Verification Method
via Mobile Number
via Email Address
via Message Service
Create Account Password
Verify Password
User Information
F64 Box Online Registration
Submit
Please input OTP before timer finishes
sent to
Submit OTP
Request new OTP
Online Regsitration Task
User Information Submitted
Requesting OTP...
Verifying OTP...
Box Successfully Registered!
Box Registration FAILED!
Server Error
PARTITION ATTRIBUTE ENHANCED
Select SoC Type of Device
Open an MTK Preloader
Check Preloader Supported eMMC / UFS
Not yet supported
Unpack other SIN files as well? 
Choose Configuration
Memory Used
RFFE Scanning in progress...
I2C Scanning in progress...
I3C Scanning in progress...
SPI Scanning in progress...
UART Scanning in progress...
Click STOP to Cancel
Common Setup
Are you sure you want to RESTART the USB?
All Running Tasks will be CANCELLED.
Continue with USB RESTART?
Are you sure you want to
STOP the current Task?
Please select a
Write CSD Register?
ERROR
PERMANENTLY WRITE PROTECT
the entire
If you are 100% sure, then click YES 3 times...
Answer this
Write RPMB Data?
This RPMB Data Write will add
to the Write Counter
Include OTP Items?
Include Write Protection Items?
Include Partition Settings Items?
Error starting discovering
Permanently Disable Firmware Update?
Are you sure you want to Set
Permanent Write Protection?
Are you sure you want to exit?
An Active Task is Running!  Exit anyway?
Test RPMB Key?
Test RPMB Write?
A successful test will add 1 to the Counter.
PERMANENTLY LOCK
the Configuration Descriptor?
Restart Application to apply Theme?
Safely Disconnect eMMC?
Finalize Partition Settings?
This procedure is One Time Programmable (OTP)
Are you sure you want to apply the changes?
Some options selected maybe OTP
Are you sure you want to Permanently disable the change 
of boot configuration register bits relating boot mode?
Reset RPMB Data and Key?
Read RPMB Key?
Factory Reset eMMC Provisioning?
This will ERASE all DATA from
and also RESET EXT_CSD settings.
Reset RPMB Counter?
Release
bytes from USER Partition?
Original
Adjusted
This procedure will make the USER Parition Smaller
Socket Information
Socket Type
Serial Number
Manufacturing Date
Activated Features
Show Box Voltages
UFS Differential Voltage Swing
I have read the EULA
I agree to the EULA
Support
Social Media
User Manual
Online Shop
Featured Accessories
Activations
Enable
Hold down CTRL key for MoviNand FFU
This will erase all DATA except RPMB
Unlock Partition Configuration
Changing Partitions will ERASE all Data (Except RPMB)! 
Partition Configuration is Locked
NTAG® Information
Programming Date
User Memory
Lock Status
Red
Green
Blue
Invert Selection
Disable
Select Backup File
Buffer Size Multiplier
Overwrite Unpacked Files?
Device Exception Level:
HID Operations:
HID Available Size:
HID Size:
HID Progress Ratio:
HID State:
WriteBooster Buffer Resize Hint Info:
WriteBooster Enable Buffer Resize:
WriteBooster Resize Op Status: 
WriteBooster Buffer Partial Flush Mode:
WriteBooster Max Partial Flush FIFO Size:
WriteBooster Current Partial Flush FIFO Size:
WriteBooster Current Pinned Buffer Allocation Size:
WriteBooster Available Pinned Buffer Size:
WriteBooster Cumulative Written Size:
WriteBooster Partial Flush Pinned Buffer Size: 
WriteBooster Partial Flush Min Non-Pinned Size:
Enable Unpin of Pinned Data:
Capacity Adjust Factor Representation Format:
Restore Previous CID
Remove Write Protect Groups
and possibly ERASE ALL DATA?
Did you already Backup Important Data?
Are you ready to say Goodbye to All Your Data?
Rescan UFS to check Write Protection Status
ERROR: Unlock bConfigDescrLock (OTP) First 
Feature not supported by this eMMC
Work Directory set to Folder
Click YES to Erase Partition with 0xFF (New Method)
Click NO to Erase Partition with 0x00 (Old Method)
Set RPMB Counter
Do you already have a Full RPMB Data Backup?
Enter Desired Counter Value
Select an RPMB Binary Backup File
RPMB Data is BLANK!
Load GPT for other Partitions?
Change Boot Slots?
Select Boot A or B
Select Proper Procedure
New Security for Android 14 and 15
FRP New Security (2024, 2025)
FRP Old Security
Partition Configuration
Reference Clock
Configuration Descriptor (OTP)
Select RPMB Read Size
Erase all LUNs
(Fix Slow UFS)
This will not erase RPMB or Write Protected Areas
Erase all Partitions
OEM Unlock
Set OEM Unlock Enable?
Erase before Write
Backup
Skip Userdata
Write to Slot A and B
Enter Custom Watermark
Slow Read/Write (For Bad UFS IC)
Resize Data Partition?
Format Partition
Select Partitions to Format
ALL DATA WILL BE GONE
Set Android Slot A
Skip eMMC Sparse File FILL
Partition Information
Partition Type GUID
Unique Partition GUID
Partition Name
First LBA
Last LBA
Flags
Apply Changes
Delete Partition
Convert BIN to SPARSE
Convert SPARSE to BIN
Trim Blank Space
Select Multiple Sparse Files
Sparsing File
Unsparsing File
Select Binary Files
Select Sparse Files
Priority
Tries Remaining
Successful
Read Only
Shadow copy
Hidden
No drive letter
Primary Connection Tasks
Post Connection Tasks
Automatic FRP Removal
Read MTK Boot Status
Read MOTO Boot Status
File Loading Option:
GPT Partitions
Single RAW Image
Check KG Info
Update KG Info
KG Status
KG RPMB Version
Erase Status Info
Erase Lock Screen Info
Erase Server Logs
Erase Metadata
Erase Secure Data
Erase Secure Token
Erase Certificate
Changing KG Status is Illegal is most Countries
Reset RAM Training
Reset RAM Training?
Erase RPMB Data
This will ERASE ALL LUNS and RPMB Data
File Tools
Script
Scripting Tool
Run Script
Use WriteBooster?
Reconnect the F64 Box
Please connect 1 F64 Box Only!
Waiting for F64 Box...
Box Detected...
Lock Script
Lock Script to F64 Box Serial Number
Select an F64 Script File
Show Larger UFS Transfer Speed
Hide Information from Logs
Check Android Verified Boot?
Hashing Data Blocks
Firmware Unpacking Tools
Dev Tools
Update Hash
Sign Android Partition
Select an Android Partition Image
This will update HASHES without making a backup.
This will update PRIVATE Key without making a backup.
Select an Android Partition Image
Updating Private Key
Select a PEM Key File
I understand that these tools are for developers only.
Android Developer
This will unpack and decompress boot files.
Select an Android Boot File
Unpack Android Boot
Select a Kernel File
Compressing File
Pack Android Boot
This will pack and overwrite files.
Are you sure you move this partition?
This will ERASE USER DATA
Move Partition
Empty Size
Erasing
Multi-File Loaded
File Loaded
Erase Success
Sector Overflow
Erase Failed
Erase Success
Not Selected
Sector Overflow
Format Success
Format Failed
Reading
Backup Success
Backup Failed
Blank Checking
Initializing...
Initializing
Formatting
Success
Partition is Blank
Not Blank
Small Size
Zero Write
PGPT Write Success
PGPT Write FAILED
SGPT Write Success
SGPT Write FAILED
Configuring GPT...
Task Skipped
MBR Write Success
MBR Write FAILED
Read Success
Read Failed
PT Write Success
PT Write FAILED
PT Backup FAILED
partinfo Write Success
partinfo Write FAILED
Repairing PT...
Repairing partinfo...
partinfo Backup FAILED
MPT Write Success
MPT Write FAILED
Repairing MPT...
Repairing MBR...
MPT Backup FAILED
MBR Backup FAILED
Write Success
Write Failed
Repartitioning MBR...
Decompressing
Decompressing...
Decompress OK
Decompress Failed
Writing
Erasing...
Writing...
Invalid File
Blank
Verifying
Verified
Not Verified
Corrupted
Checking AVB Footer
Erase Only
File Loaded
Updating MBR...
Updating GPT...
OEM Unlock
OEM Unlock Failed
OEM Unlock Success
Patching
... double-click to add file ...
Left Mouse Button
Single Click + Hold : Drag Image
Double Click : Load New Image
Middle Scroll Wheel
Scroll Up : Zoom In (+ SHIFT KEY : Faster, + CTRL KEY : Slower)
Scroll Down : Zoom Out (+ SHIFT KEY : Faster, + CTRL KEY : Slower)
Right Mouse Button
Rotate Clockwise (+ SHIFT KEY : Rotate Counter Clockwise)
HEX View Partition
Are you sure you want to HEX View Partition?
Go to Offset
Enter Offset
Maximum
Hex
Decimal
Text-string
Hex-values
Search for
Replace with
Options
Text encoding
Case sensitive
Prompt on replace
Search direction
All
Forward
Backward
OK
Replace all
Cancel
Find
Value not found
No previous occurrence found
Pattern cannot be empty
Replace
Strings must have same length
Pattern length mismatch
Pattern cannot be empty
Replace this occurrence?
Replace Error
Undo
Clipboard Limit
Click to reveal location
Copy
Copy Text
Paste
Fill selection
Select all
Find
Replace
Find again
Find again (reversed)
Go to
Fill selection
Fill pattern
Please enter a valid hex pattern
Pattern is too long (Max 32768 bytes)
Pattern exceeds selection size.
Max allowed bytes for this selection
Min range must be between 0 and 255
Max range must be between 0 and 255
Min value cannot be greater than Max value
Random bytes
Range (decimal)
Error
Selection too large to copy
Maximum
Minimum
Average