arch	circuit	script_params	vtr_flow_elapsed_time	vtr_max_mem_stage	vtr_max_mem	error	odin_synth_time	max_odin_mem	parmys_synth_time	max_parmys_mem	abc_depth	abc_synth_time	abc_cec_time	abc_sec_time	max_abc_mem	ace_time	max_ace_mem	num_clb	num_io	num_memories	num_mult	vpr_status	vpr_revision	vpr_build_info	vpr_compiler	vpr_compiled	hostname	rundir	max_vpr_mem	num_primary_inputs	num_primary_outputs	num_pre_packed_nets	num_pre_packed_blocks	num_netlist_clocks	num_post_packed_nets	num_post_packed_blocks	device_width	device_height	device_grid_tiles	device_limiting_resources	device_name	pack_mem	pack_time	initial_placed_wirelength_est	placed_wirelength_est	total_swap	accepted_swap	rejected_swap	aborted_swap	place_mem	place_time	place_quench_time	initial_placed_CPD_est	placed_CPD_est	placed_setup_TNS_est	placed_setup_WNS_est	placed_geomean_nonvirtual_intradomain_critical_path_delay_est	place_delay_matrix_lookup_time	place_quench_timing_analysis_time	place_quench_sta_time	place_total_timing_analysis_time	place_total_sta_time	ap_mem	ap_time	ap_full_legalizer_mem	ap_full_legalizer_time	routed_wirelength	avg_routed_wirelength	routed_wiresegment	avg_routed_wiresegment	total_nets_routed	total_connections_routed	total_heap_pushes	total_heap_pops	logic_block_area_total	logic_block_area_used	routing_area_total	routing_area_per_tile	crit_path_route_success_iteration	num_rr_graph_nodes	num_rr_graph_edges	collapsed_nodes	critical_path_delay	geomean_nonvirtual_intradomain_critical_path_delay	setup_TNS	setup_WNS	hold_TNS	hold_WNS	create_rr_graph_time	create_intra_cluster_rr_graph_time	adding_internal_edges	route_mem	crit_path_route_time	crit_path_total_timing_analysis_time	crit_path_total_sta_time	router_lookahead_mem	tile_lookahead_computation_time	router_lookahead_computation_time	
k6_frac_N10_frac_chain_mem32K_40nm.xml	sha.v	common	3.90	vpr	81.28 MiB		-1	-1	0.63	49260	4	0.71	-1	-1	39880	-1	-1	130	38	0	0	success	6527d14ed	release IPO VTR_ASSERT_LEVEL=2	GNU 13.3.0 on Linux-6.8.0-84-generic x86_64	2026-03-14T16:18:18	KingsLanding	/home/pliebste/vtr-verilog-to-routing	83232	38	36	2741	2490	1	1029	204	15	15	225	clb	auto	45.5 MiB	0.95	13875.5	8340	57204	21844	34143	1217	81.3 MiB	0.51	0.01	10.5758	8.99751	-2532.5	-8.99751	8.99751	0.00	0.00188567	0.00171354	0.207952	0.185	-1	-1	-1	-1	10409	10.1452	2896	2.82261	3044	6551	310089	44471	1.03862e+07	7.00622e+06	3.52643e+06	15673.0	18	49558	600182	-1	9.49135	9.49135	-2689.22	-9.49135	0	0	0.32	-1	-1	81.3 MiB	0.14	0.321615	0.290326	81.3 MiB	-1	0.07	
