#VPR Min W Routing Metrics
min_chan_width;vpr.out;Best routing used a channel width factor of (\d+)
routed_wirelength;vpr.out;\s*Total wirelength: (.*), average .*
min_chan_width_route_success_iteration;vpr.out;Successfully routed after (\d+) routing iterations

logic_block_area_total;vpr.out;\s*Total logic block area .*: (.*)
logic_block_area_used;vpr.out;\s*Total used logic block area: (.*)
min_chan_width_routing_area_total;vpr.out;\s*Total routing area: (.*), per logic tile: .*
min_chan_width_routing_area_per_tile;vpr.out;\s*Total routing area: .*, per logic tile: (.*)

#VPR Run-time Metrics
min_chan_width_route_time;vpr.out;\s*Routing took (.*) seconds .*
