#
############################################
# Configuration file for running experiments
##############################################

# Path to directory of circuits to use
circuits_dir=benchmarks/blif/4

# Path to directory of architectures to use
archs_dir=arch/bidir

# Add circuits to list to sweep
circuit_list_add=alu4.blif
circuit_list_add=apex2.blif
circuit_list_add=apex4.blif
circuit_list_add=bigkey.blif
circuit_list_add=clma.blif
circuit_list_add=des.blif
circuit_list_add=diffeq.blif
circuit_list_add=dsip.blif
circuit_list_add=elliptic.blif
circuit_list_add=ex1010.blif
circuit_list_add=ex5p.blif
circuit_list_add=frisc.blif
circuit_list_add=misex3.blif
circuit_list_add=pdc.blif
circuit_list_add=s298.blif
circuit_list_add=s38417.blif
circuit_list_add=s38584.1.blif
circuit_list_add=seq.blif
circuit_list_add=spla.blif
circuit_list_add=tseng.blif

# Add architectures to list to sweep
arch_list_add=k4_n4_v7_bidir.xml
arch_list_add=k4_n4_v7_l1_bidir.xml

# Parse info and how to parse
parse_file=vpr_standard.txt

# How to parse QoR info
qor_parse_file=qor_standard.txt

# Pass requirements
pass_requirements_file=pass_requirements.txt

#We increase the critical path router iterations beyond the default 50, to avoid
#spurrious routing failures at relaxed channel width (since we know they should 
#be routable via the minimum channel width search)
script_params=-starting_stage vpr -track_memory_usage -crit_path_router_iterations 60 --seed 250

