#VPR metrics at fixed channel width with timing
%include "../common/pass_requirements.vpr_route_fixed_chan_width.txt"

#Timing metrics
critical_path_delay;Range(0.50,1.40)
geomean_nonvirtual_intradomain_critical_path_delay;Range(0.50,1.40)
setup_TNS;Range(0.50,1.40)
setup_WNS;Range(0.50,1.40)
#hold_TNS;Range(0.05,20.00)
#hold_WNS;Range(0.05,20.00)
