##############################################
# Configuration file for running experiments
##############################################

# Path to directory of circuits to use
circuits_dir=benchmarks/noc/Synthetic_Designs/blif_files/

# Path to directory of architectures to use
archs_dir=arch/noc/mesh_noc_topology

# Path to directory of NoC Traffic Patterns to use
noc_traffics_dir=benchmarks/noc/Synthetic_Designs/traffic_flow_files/

# Traffic flow files are added per circuit.
# By default, the task performs a cartesian product between circuits and traffic flow files.
# Since each circuit is compatible with specific traffic flow files, we need to specify
# traffic flow files for each circuit separately.
noc_traffic_list_type=per_circuit

# Add circuits and traffic flows to list to sweep
circuit_list_add=simple_16_noc_1D_chain.blif
noc_traffic_list_add=simple_16_noc_1D_chain.flows

circuit_list_add=simple_32_noc_clique.blif
noc_traffic_list_add=simple_32_noc_clique.flows

circuit_list_add=simple_32_noc_star.blif
noc_traffic_list_add=simple_32_noc_star.flows
circuit_list_add=simple_32_noc_star.blif
noc_traffic_list_add=simple_32_noc_star_no_constraints.flows

circuit_list_add=simple_64_noc_clique.blif
noc_traffic_list_add=simple_64_noc_clique.flows

circuit_list_add=simple_64_noc_2D_chain.blif
noc_traffic_list_add=simple_64_noc_2D_chain.flows

circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_12_latency_constraints.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_24_latency_constraints.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_2_bandwidths.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_3_bandwidths.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_40_latency_constraints.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_4_bandwidths.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_4_latency_constraints.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_58_latency_constraints.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_5_bandwidths.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_63_latency_constraints.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_6_bandwidths.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star.flows
circuit_list_add=simple_64_noc_star.blif
noc_traffic_list_add=simple_64_noc_star_no_constraints.flows

# Add architectures to list to sweep
arch_list_add=stratixiv_arch.timing_with_a_embedded_10X10_mesh_noc_topology.xml

# Parse info and how to parse
parse_file=vpr_noc.txt

# How to parse QoR info
qor_parse_file=qor_noc_spec.txt

# Pass requirements
#pass_requirements_file=

# Script parameters
script_params_common =-starting_stage vpr --noc on --noc_routing_algorithm xy_routing --device "EP4SE820"
