#
############################################
# Configuration file for running experiments
##############################################

# Path to directory of circuits to use
circuits_dir=benchmarks/verilog

# Path to directory of architectures to use
archs_dir=arch/complex_switch

# Add circuits to list to sweep
circuit_list_add=bgm.v
circuit_list_add=blob_merge.v
circuit_list_add=boundtop.v
circuit_list_add=LU8PEEng.v
circuit_list_add=mkDelayWorker32B.v
circuit_list_add=mkSMAdapter4B.v
circuit_list_add=or1200.v
circuit_list_add=raygentop.v
circuit_list_add=sha.v
circuit_list_add=stereovision0.v
circuit_list_add=stereovision1.v
circuit_list_add=stereovision2.v
circuit_list_add=LU32PEEng.v
circuit_list_add=mcml.v

# Add architectures to list to sweep
arch_list_add=k4_N8_topology-0.85sL2-0.15gL4-on-cb-off-sb_22nm_22nm.xml

# Parse info and how to parse
parse_file=vpr_fixed_chan_width.txt

# How to parse QoR info
qor_parse_file=qor_fixed_chan_width.txt

# Pass requirements
pass_requirements_file=pass_requirements_fixed_chan_width.txt

script_params= -start odin -track_memory_usage --route_chan_width 200

