<style>
  .tooltip {
    padding: 15px;
    border-radius: 5px;
    margin-bottom: 10px;
    display: flex;
    align-items: center;
  }

  .tooltip .icon {
    font-size: 1rem;
    margin-right: 10px;
  }

  .tip {
    background-color: #fcf003;
    color: #333;
  }

  .warning {
    background-color: #ffb3b3;
    color: #333;
  }

  .info {
    background-color: #cce5ff;
    color: #004085;
  }

  .info a {
    color: #004085;
    font-weight: bold;
    text-decoration: underline;
  }
</style>


## Step 1: Prepare necessary tools

- A #1 Phillips head screwdriver

![](../img/1.JPG)


## Step 2: Place PCB into Base

<div class="tooltip tip">
  <span class="icon">💡</span>
  <span><strong>Tip:</strong> The PCB may require a bit of force to get in.</span>
</div>

![](../img/2.jpg)

## Step 3: Insert Magnet into Spring

<div class="tooltip tip">
  <span class="icon">💡</span>
  <span><strong>Tip:</strong> The magnet must be inserted with the <b>north</b> side facing <b>upwards</b>. Use a compass to determine the orientation of the magnet.</span>
</div>

- The magnet requires a bit of force to fully insert.
- Once inserted, the Magnet will be very difficult to remove.

![](../img/3.jpg)

## Step 4: Place Friction Nub onto Spring

![](../img/4.jpg)

- If you want to 3D-print your own nub, you can use [this free design to do so](https://makerworld.com/en/models/483268-trackpoint-cap-for-thinkpad-keyboard#profileId-402360).

## Step 5: Place Spring into Top

<div class="tooltip tip">
  <span class="icon">💡</span>
  <span><strong>Tip:</strong> The Spring must be oriented correctly in order to properly insert. See the photo for details.</span>
</div>

![](../img/5.jpg)

## Step 6: Place Top onto Base

<div class="tooltip tip">
  <span class="icon">💡</span>
  <span><strong>Tip:</strong> The Top should snap into place on the Base.</span>
</div>

![](../img/6.jpg)

## Step 7: Screw Top to Base

![](../img/7.jpg)

## Step 8: Place Friction Pads on Base

![](../img/8.jpg)

## Step 9: All done!

![](../img/9.jpg)

## Post Build Steps:

### Verify the device is working correctly

- Plug the Bean into the computer using a USB-C cable
- Move the nub around, it should move the cursor
- Press each of the buttons to verify their function

<div class="tooltip info">
  <span class="icon">ℹ️</span>
  <span><strong>Info:</strong> The default keymap for the Bean is <a href="../appendices/keymap/">here</a>.</span>
</div>

### Check out Post Build FAQ
- [Post Build FAQ](https://help.ploopy.co/?docs=where-can-i-find-mods-for-my-ploopy-device)
- Contains various information about things you can do after initial assembly!

<div class="tooltip info">
  <span class="icon">ℹ️</span>
  <span><strong>Info:</strong> If the device is not working, consult our <a href="https://help.ploopy.co/checklist-v2/">troubleshooting guide</a> for further steps.
</div>



<!--
<div class="tooltip tip">
  <span class="icon">💡</span>
  <span><strong>Tip:</strong> Here's an interesting piece of info!</span>
</div>

<div class="tooltip warning">
  <span class="icon">🚨</span>
  <span><strong>Warning:</strong> Here's a warning!</span>
</div>

<div class="tooltip info">
  <span class="icon">ℹ️</span>
  <span><strong>Info:</strong> Here's some cool stuff!</span>
</div>
-->
