@chapter Input Devices
@c man begin INPUT DEVICES

Input devices are configured elements in FFmpeg which enable accessing
the data coming from a multimedia device attached to your system.

When you configure your FFmpeg build, all the supported input devices
are enabled by default. You can list all available ones using the
configure option "--list-indevs".

You can disable all the input devices using the configure option
"--disable-indevs", and selectively enable an input device using the
option "--enable-indev=@var{INDEV}", or you can disable a particular
input device using the option "--disable-indev=@var{INDEV}".

The option "-devices" of the ff* tools will display the list of
supported input devices.

A description of the currently available input devices follows.

@section alsa

ALSA (Advanced Linux Sound Architecture) input device.

To enable this input device during configuration you need libasound
installed on your system.

This device allows capturing from an ALSA device. The name of the
device to capture has to be an ALSA card identifier.

An ALSA identifier has the syntax:
@example
hw:@var{CARD}[,@var{DEV}[,@var{SUBDEV}]]
@end example

where the @var{DEV} and @var{SUBDEV} components are optional.

The three arguments (in order: @var{CARD},@var{DEV},@var{SUBDEV})
specify card number or identifier, device number and subdevice number
(-1 means any).

To see the list of cards currently recognized by your system check the
files @file{/proc/asound/cards} and @file{/proc/asound/devices}.

For example to capture with @command{ffmpeg} from an ALSA device with
card id 0, you may run the command:
@example
ffmpeg -f alsa -i hw:0 alsaout.wav
@end example

For more information see:
@url{http://www.alsa-project.org/alsa-doc/alsa-lib/pcm.html}

@subsection Options

@table @option

@item sample_rate
Set the sample rate in Hz. Default is 48000.

@item channels
Set the number of channels. Default is 2.

@end table

@section android_camera

Android camera input device.

This input devices uses the Android Camera2 NDK API which is
available on devices with API level 24+. The availability of
android_camera is autodetected during configuration.

This device allows capturing from all cameras on an Android device,
which are integrated into the Camera2 NDK API.

The available cameras are enumerated internally and can be selected
with the @var{camera_index} parameter. The input file string is
discarded.

Generally the back facing camera has index 0 while the front facing
camera has index 1.

@subsection Options

@table @option

@item video_size
Set the video size given as a string such as 640x480 or hd720.
Falls back to the first available configuration reported by
Android if requested video size is not available or by default.

@item framerate
Set the video framerate.
Falls back to the first available configuration reported by
Android if requested framerate is not available or by default (-1).

@item camera_index
Set the index of the camera to use. Default is 0.

@item input_queue_size
Set the maximum number of frames to buffer. Default is 5.

@end table

@section avfoundation

AVFoundation input device.

AVFoundation is the currently recommended framework by Apple for streamgrabbing on OSX >= 10.7 as well as on iOS.

The input filename has to be given in the following syntax:
@example
-i "[[VIDEO]:[AUDIO]]"
@end example
The first entry selects the video input while the latter selects the audio input.
The stream has to be specified by the device name or the device index as shown by the device list.
Alternatively, the video and/or audio input device can be chosen by index using the
@option{
    -video_device_index <INDEX>
}
and/or
@option{
    -audio_device_index <INDEX>
}
, overriding any
device name or index given in the input filename.

All available devices can be enumerated by using @option{-list_devices true}, listing
all device names and corresponding indices.

There are two device name aliases:
@table @code

@item default
Select the AVFoundation default device of the corresponding type.

@item none
Do not record the corresponding media type.
This is equivalent to specifying an empty device name or index.

@end table

@subsection Options

AVFoundation supports the following options:

@table @option

@item -list_devices <TRUE|FALSE>
If set to true, a list of all available input devices is given showing all
device names and indices.

@item -video_device_index <INDEX>
Specify the video device by its index. Overrides anything given in the input filename.

@item -audio_device_index <INDEX>
Specify the audio device by its index. Overrides anything given in the input filename.

@item -pixel_format <FORMAT>
Request the video device to use a specific pixel format.
If the specified format is not supported, a list of available formats is given
and the first one in this list is used instead. Available pixel formats are:
@code{monob, rgb555be, rgb555le, rgb565be, rgb565le, rgb24, bgr24, 0rgb, bgr0, 0bgr, rgb0,
 bgr48be, uyvy422, yuva444p, yuva444p16le, yuv444p, yuv422p16, yuv422p10, yuv444p10,
 yuv420p, nv12, yuyv422, gray}

@item -framerate
Set the grabbing frame rate. Default is @code{ntsc}, corresponding to a
frame rate of @code{30000/1001}.

@item -video_size
Set the video frame size.

@item -capture_cursor
Capture the mouse pointer. Default is 0.

@item -capture_mouse_clicks
Capture the screen mouse clicks. Default is 0.

@item -capture_raw_data
Capture the raw device data. Default is 0.
Using this option may result in receiving the underlying data delivered to the AVFoundation framework. E.g. for muxed devices that sends raw DV data to the framework (like tape-based camcorders), setting this option to false results in extracted video frames captured in the designated pixel format only. Setting this option to true results in receiving the raw DV stream untouched.
@end table

@subsection Examples

@itemize

@item
Print the list of AVFoundation supported devices and exit:
@example
$ ffmpeg -f avfoundation -list_devices true -i ""
@end example

@item
Record video from video device 0 and audio from audio device 0 into out.avi:
@example
$ ffmpeg -f avfoundation -i "0:0" out.avi
@end example

@item
Record video from video device 2 and audio from audio device 1 into out.avi:
@example
$ ffmpeg -f avfoundation -video_device_index 2 -i ":1" out.avi
@end example

@item
Record video from the system default video device using the pixel format bgr0 and do not record any audio into out.avi:
@example
$ ffmpeg -f avfoundation -pixel_format bgr0 -i "default:none" out.avi
@end example

@item
Record raw DV data from a suitable input device and write the output into out.dv:
@example
$ ffmpeg -f avfoundation -capture_raw_data true -i "zr100:none" out.dv
@end example


@end itemize

@section decklink

The decklink input device provides capture capabilities for Blackmagic
DeckLink devices.

To enable this input device, you need the Blackmagic DeckLink SDK and you
need to configure with the appropriate @code{--extra-cflags}
and @code{--extra-ldflags}.
On Windows, you need to run the IDL files through @command{widl}.

DeckLink is very picky about the formats it supports. Pixel format of the
input can be set with @option{raw_format}.
Framerate and video size must be determined for your device with
@command{-list_formats 1}. Audio sample rate is always 48 kHz and the number
of channels can be 2, 8 or 16. Note that all audio channels are bundled in one single
audio track.

@subsection Options

@table @option

@item list_devices
If set to @option{true}, print a list of devices and exit.
Defaults to @option{false}. This option is deprecated, please use the
@code{-sources} option of ffmpeg to list the available input devices.

@item list_formats
If set to @option{true}, print a list of supported formats and exit.
Defaults to @option{false}.

@item format_code <FourCC>
This sets the input video format to the format given by the FourCC. To see
the supported values of your device(s) use @option{list_formats}.
Note that there is a FourCC @option{'pal '} that can also be used
as @option{pal} (3 letters).
Default behavior is autodetection of the input video format, if the hardware
supports it.

@item raw_format
Set the pixel format of the captured video.
Available values are:
@table @samp
@item auto

This is the default which means 8-bit YUV 422 or 8-bit ARGB if format
autodetection is used, 8-bit YUV 422 otherwise.

@item uyvy422

8-bit YUV 422.

@item yuv422p10

10-bit YUV 422.

@item argb

8-bit RGB.

@item bgra

8-bit RGB.

@item rgb10

10-bit RGB.

@end table

@item teletext_lines
If set to nonzero, an additional teletext stream will be captured from the
vertical ancillary data. Both SD PAL (576i) and HD (1080i or 1080p)
sources are supported. In case of HD sources, OP47 packets are decoded.

This option is a bitmask of the SD PAL VBI lines captured, specifically lines 6
to 22, and lines 318 to 335. Line 6 is the LSB in the mask. Selected lines
which do not contain teletext information will be ignored. You can use the
special @option{all} constant to select all possible lines, or
@option{standard} to skip lines 6, 318 and 319, which are not compatible with
all receivers.

For SD sources, ffmpeg needs to be compiled with @code{--enable-libzvbi}. For
HD sources, on older (pre-4K) DeckLink card models you have to capture in 10
bit mode.

@item channels
Defines number of audio channels to capture. Must be @samp{2}, @samp{8} or @samp{16}.
Defaults to @samp{2}.

@item duplex_mode
Sets the decklink device duplex/profile mode. Must be @samp{unset}, @samp{half}, @samp{full},
@samp{one_sub_device_full}, @samp{one_sub_device_half}, @samp{two_sub_device_full},
@samp{four_sub_device_half}
Defaults to @samp{unset}.

Note: DeckLink SDK 11.0 have replaced the duplex property by a profile property.
For the DeckLink Duo 2 and DeckLink Quad 2, a profile is shared between any 2
sub-devices that utilize the same connectors. For the DeckLink 8K Pro, a profile
is shared between all 4 sub-devices. So DeckLink 8K Pro support four profiles.

Valid profile modes for DeckLink 8K Pro(with DeckLink SDK >= 11.0):
@samp{one_sub_device_full}, @samp{one_sub_device_half}, @samp{two_sub_device_full},
@samp{four_sub_device_half}

Valid profile modes for DeckLink Quad 2 and DeckLink Duo 2:
@samp{half}, @samp{full}

@item timecode_format
Timecode type to include in the frame and video stream metadata. Must be
@samp{none}, @samp{rp188vitc}, @samp{rp188vitc2}, @samp{rp188ltc},
@samp{rp188hfr}, @samp{rp188any}, @samp{vitc}, @samp{vitc2}, or @samp{serial}.
Defaults to @samp{none} (not included).

In order to properly support 50/60 fps timecodes, the ordering of the queried
timecode types for @samp{rp188any} is HFR, VITC1, VITC2 and LTC for >30 fps
content. Note that this is slightly different to the ordering used by the
DeckLink API, which is HFR, VITC1, LTC, VITC2.

@item video_input
Sets the video input source. Must be @samp{unset}, @samp{sdi}, @samp{hdmi},
@samp{optical_sdi}, @samp{component}, @samp{composite} or @samp{s_video}.
Defaults to @samp{unset}.

@item audio_input
Sets the audio input source. Must be @samp{unset}, @samp{embedded},
@samp{aes_ebu}, @samp{analog}, @samp{analog_xlr}, @samp{analog_rca} or
@samp{microphone}. Defaults to @samp{unset}.

@item video_pts
Sets the video packet timestamp source. Must be @samp{video}, @samp{audio},
@samp{reference}, @samp{wallclock} or @samp{abs_wallclock}.
Defaults to @samp{video}.

@item audio_pts
Sets the audio packet timestamp source. Must be @samp{video}, @samp{audio},
@samp{reference}, @samp{wallclock} or @samp{abs_wallclock}.
Defaults to @samp{audio}.

@item draw_bars
If set to @samp{true}, color bars are drawn in the event of a signal loss.
Defaults to @samp{true}.
This option is deprecated, please use the @code{signal_loss_action} option.

@item signal_loss_action
Sets the action to take in the event of a signal loss. Accepts one of the
following values:

@table @option
@item 1, none
Do nothing on signal loss. This usually results in black frames.
@item 2, bars
Draw color bars on signal loss. Only supported for 8-bit input signals.
@item 3, repeat
Repeat the last video frame on signal loss.
@end table

Defaults to @samp{bars}.

@item queue_size
Sets maximum input buffer size in bytes. If the buffering reaches this value,
incoming frames will be dropped.
Defaults to @samp{1073741824}.

@item audio_depth
Sets the audio sample bit depth. Must be @samp{16} or @samp{32}.
Defaults to @samp{16}.

@item decklink_copyts
If set to @option{true}, timestamps are forwarded as they are without removing
the initial offset.
Defaults to @option{false}.

@item timestamp_align
Capture start time alignment in seconds. If set to nonzero, input frames are
dropped till the system timestamp aligns with configured value.
Alignment difference of up to one frame duration is tolerated.
This is useful for maintaining input synchronization across N different
hardware devices deployed for 'N-way' redundancy. The system time of different
hardware devices should be synchronized with protocols such as NTP or PTP,
before using this option.
Note that this method is not foolproof. In some border cases input
synchronization may not happen due to thread scheduling jitters in the OS.
Either sync could go wrong by 1 frame or in a rarer case
@option{timestamp_align} seconds.
Defaults to @samp{0}.

@item wait_for_tc (@emph{bool})
Drop frames till a frame with timecode is received. Sometimes serial timecode
isn't received with the first input frame. If that happens, the stored stream
timecode will be inaccurate. If this option is set to @option{true}, input frames
are dropped till a frame with timecode is received.
Option @var{timecode_format} must be specified.
Defaults to @option{false}.

@item enable_klv(@emph{bool})
If set to @option{true}, extracts KLV data from VANC and outputs KLV packets.
KLV VANC packets are joined based on MID and PSC fields and aggregated into
one KLV packet.
Defaults to @option{false}.

@end table

@subsection Examples

@itemize

@item
List input devices:
@example
ffmpeg -sources decklink
@end example

@item
List supported formats:
@example
ffmpeg -f decklink -list_formats 1 -i 'Intensity Pro'
@end example

@item
Capture video clip at 1080i50:
@example
ffmpeg -format_code Hi50 -f decklink -i 'Intensity Pro' -c:a copy -c:v copy output.avi
@end example

@item
Capture video clip at 1080i50 10 bit:
@example
ffmpeg -raw_format yuv422p10 -format_code Hi50 -f decklink -i 'UltraStudio Mini Recorder' -c:a copy -c:v copy output.avi
@end example

@item
Capture video clip at 1080i50 with 16 audio channels:
@example
ffmpeg -channels 16 -format_code Hi50 -f decklink -i 'UltraStudio Mini Recorder' -c:a copy -c:v copy output.avi
@end example

@end itemize

@section dshow

Windows DirectShow input device.

DirectShow support is enabled when FFmpeg is built with the mingw-w64 project.
Currently only audio and video devices are supported.

Multiple devices may be opened as separate inputs, but they may also be
opened on the same input, which should improve synchronism between them.

The input name should be in the format:

@example
@var{TYPE}=@var{NAME}[:@var{TYPE}=@var{NAME}]
@end example

where @var{TYPE} can be either @var{audio} or @var{video},
and @var{NAME} is the device's name or alternative name..

@subsection Options

If no options are specified, the device's defaults are used.
If the device does not support the requested options, it will
fail to open.

@table @option

@item video_size
Set the video size in the captured video.

@item framerate
Set the frame rate in the captured video.

@item sample_rate
Set the sample rate (in Hz) of the captured audio.

@item sample_size
Set the sample size (in bits) of the captured audio.

@item channels
Set the number of channels in the captured audio.

@item list_devices
If set to @option{true}, print a list of devices and exit.

@item list_options
If set to @option{true}, print a list of selected device's options
and exit.

@item video_device_number
Set video device number for devices with the same name (starts at 0,
defaults to 0).

@item audio_device_number
Set audio device number for devices with the same name (starts at 0,
defaults to 0).

@item pixel_format
Select pixel format to be used by DirectShow. This may only be set when
the video codec is not set or set to rawvideo.

@item audio_buffer_size
Set audio device buffer size in milliseconds (which can directly
impact latency, depending on the device).
Defaults to using the audio device's
default buffer size (typically some multiple of 500ms).
Setting this value too low can degrade performance.
See also
@url{http://msdn.microsoft.com/en-us/library/windows/desktop/dd377582(v=vs.85).aspx}

@item video_pin_name
Select video capture pin to use by name or alternative name.

@item audio_pin_name
Select audio capture pin to use by name or alternative name.

@item crossbar_video_input_pin_number
Select video input pin number for crossbar device. This will be
routed to the crossbar device's Video Decoder output pin.
Note that changing this value can affect future invocations
(sets a new default) until system reboot occurs.

@item crossbar_audio_input_pin_number
Select audio input pin number for crossbar device. This will be
routed to the crossbar device's Audio Decoder output pin.
Note that changing this value can affect future invocations
(sets a new default) until system reboot occurs.

@item show_video_device_dialog
If set to @option{true}, before capture starts, popup a display dialog
to the end user, allowing them to change video filter properties
and configurations manually.
Note that for crossbar devices, adjusting values in this dialog
may be needed at times to toggle between PAL (25 fps) and NTSC (29.97)
input frame rates, sizes, interlacing, etc.  Changing these values can
enable different scan rates/frame rates and avoiding green bars at
the bottom, flickering scan lines, etc.
Note that with some devices, changing these properties can also affect future
invocations (sets new defaults) until system reboot occurs.

@item show_audio_device_dialog
If set to @option{true}, before capture starts, popup a display dialog
to the end user, allowing them to change audio filter properties
and configurations manually.

@item show_video_crossbar_connection_dialog
If set to @option{true}, before capture starts, popup a display
dialog to the end user, allowing them to manually
modify crossbar pin routings, when it opens a video device.

@item show_audio_crossbar_connection_dialog
If set to @option{true}, before capture starts, popup a display
dialog to the end user, allowing them to manually
modify crossbar pin routings, when it opens an audio device.

@item show_analog_tv_tuner_dialog
If set to @option{true}, before capture starts, popup a display
dialog to the end user, allowing them to manually
modify TV channels and frequencies.

@item show_analog_tv_tuner_audio_dialog
If set to @option{true}, before capture starts, popup a display
dialog to the end user, allowing them to manually
modify TV audio (like mono vs. stereo, Language A,B or C).

@item audio_device_load
Load an audio capture filter device from file instead of searching
it by name. It may load additional parameters too, if the filter
supports the serialization of its properties to.
To use this an audio capture source has to be specified, but it can
be anything even fake one.

@item audio_device_save
Save the currently used audio capture filter device and its
parameters (if the filter supports it) to a file.
If a file with the same name exists it will be overwritten.

@item video_device_load
Load a video capture filter device from file instead of searching
it by name. It may load additional parameters too, if the filter
supports the serialization of its properties to.
To use this a video capture source has to be specified, but it can
be anything even fake one.

@item video_device_save
Save the currently used video capture filter device and its
parameters (if the filter supports it) to a file.
If a file with the same name exists it will be overwritten.

@item use_video_device_timestamps
If set to @option{false}, the timestamp for video frames will be
derived from the wallclock instead of the timestamp provided by
the capture device. This allows working around devices that
provide unreliable timestamps.

@end table

@subsection Examples

@itemize

@item
Print the list of DirectShow supported devices and exit:
@example
$ ffmpeg -list_devices true -f dshow -i dummy
@end example

@item
Open video device @var{Camera}:
@example
$ ffmpeg -f dshow -i video="Camera"
@end example

@item
Open second video device with name @var{Camera}:
@example
$ ffmpeg -f dshow -video_device_number 1 -i video="Camera"
@end example

@item
Open video device @var{Camera} and audio device @var{Microphone}:
@example
$ ffmpeg -f dshow -i video="Camera":audio="Microphone"
@end example

@item
Print the list of supported options in selected device and exit:
@example
$ ffmpeg -list_options true -f dshow -i video="Camera"
@end example

@item
Specify pin names to capture by name or alternative name, specify alternative device name:
@example
$ ffmpeg -f dshow -audio_pin_name "Audio Out" -video_pin_name 2 -i video=video="@@device_pnp_\\?\pci#ven_1a0a&dev_6200&subsys_62021461&rev_01#4&e2c7dd6&0&00e1#@{65e8773d-8f56-11d0-a3b9-00a0c9223196@}\@{ca465100-deb0-4d59-818f-8c477184adf6@}":audio="Microphone"
@end example

@item
Configure a crossbar device, specifying crossbar pins, allow user to adjust video capture properties at startup:
@example
$ ffmpeg -f dshow -show_video_device_dialog true -crossbar_video_input_pin_number 0
     -crossbar_audio_input_pin_number 3 -i video="AVerMedia BDA Analog Capture":audio="AVerMedia BDA Analog Capture"
@end example

@end itemize

@section fbdev

Linux framebuffer input device.

The Linux framebuffer is a graphic hardware-independent abstraction
layer to show graphics on a computer monitor, typically on the
console. It is accessed through a file device node, usually
@file{/dev/fb0}.

For more detailed information read the file
Documentation/fb/framebuffer.txt included in the Linux source tree.

See also @url{http://linux-fbdev.sourceforge.net/}, and fbset(1).

To record from the framebuffer device @file{/dev/fb0} with
@command{ffmpeg}:
@example
ffmpeg -f fbdev -framerate 10 -i /dev/fb0 out.avi
@end example

You can take a single screenshot image with the command:
@example
ffmpeg -f fbdev -framerate 1 -i /dev/fb0 -frames:v 1 screenshot.jpeg
@end example

@subsection Options

@table @option

@item framerate
Set the frame rate. Default is 25.

@end table

@section gdigrab

Win32 GDI-based screen capture device.

This device allows you to capture a region of the display on Windows.

Amongst options for the input filenames are such elements as:
@example
desktop
@end example
or
@example
title=@var{window_title}
@end example
or
@example
hwnd=@var{window_hwnd}
@end example

The first option will capture the entire desktop, or a fixed region of the
desktop. The second and third options will instead capture the contents of a single
window, regardless of its position on the screen.

For example, to grab the entire desktop using @command{ffmpeg}:
@example
ffmpeg -f gdigrab -framerate 6 -i desktop out.mpg
@end example

Grab a 640x480 region at position @code{10,20}:
@example
ffmpeg -f gdigrab -framerate 6 -offset_x 10 -offset_y 20 -video_size vga -i desktop out.mpg
@end example

Grab the contents of the window named "Calculator"
@example
ffmpeg -f gdigrab -framerate 6 -i title=Calculator out.mpg
@end example

@subsection Options

@table @option
@item draw_mouse
Specify whether to draw the mouse pointer. Use the value @code{0} to
not draw the pointer. Default value is @code{1}.

@item framerate
Set the grabbing frame rate. Default value is @code{ntsc},
corresponding to a frame rate of @code{30000/1001}.

@item show_region
Show grabbed region on screen.

If @var{show_region} is specified with @code{1}, then the grabbing
region will be indicated on screen. With this option, it is easy to
know what is being grabbed if only a portion of the screen is grabbed.

Note that @var{show_region} is incompatible with grabbing the contents
of a single window.

For example:
@example
ffmpeg -f gdigrab -show_region 1 -framerate 6 -video_size cif -offset_x 10 -offset_y 20 -i desktop out.mpg
@end example

@item video_size
Set the video frame size. The default is to capture the full screen if @file{desktop} is selected, or the full window size if @file{title=@var{window_title}} is selected.

@item offset_x
When capturing a region with @var{video_size}, set the distance from the left edge of the screen or desktop.

Note that the offset calculation is from the top left corner of the primary monitor on Windows. If you have a monitor positioned to the left of your primary monitor, you will need to use a negative @var{offset_x} value to move the region to that monitor.

@item offset_y
When capturing a region with @var{video_size}, set the distance from the top edge of the screen or desktop.

Note that the offset calculation is from the top left corner of the primary monitor on Windows. If you have a monitor positioned above your primary monitor, you will need to use a negative @var{offset_y} value to move the region to that monitor.

@end table

@section iec61883

FireWire DV/HDV input device using libiec61883.

To enable this input device, you need libiec61883, libraw1394 and
libavc1394 installed on your system. Use the configure option
@code{--enable-libiec61883} to compile with the device enabled.

The iec61883 capture device supports capturing from a video device
connected via IEEE1394 (FireWire), using libiec61883 and the new Linux
FireWire stack (juju). This is the default DV/HDV input method in Linux
Kernel 2.6.37 and later, since the old FireWire stack was removed.

Specify the FireWire port to be used as input file, or "auto"
to choose the first port connected.

@subsection Options

@table @option

@item dvtype
Override autodetection of DV/HDV. This should only be used if auto
detection does not work, or if usage of a different device type
should be prohibited. Treating a DV device as HDV (or vice versa) will
not work and result in undefined behavior.
The values @option{auto}, @option{dv} and @option{hdv} are supported.

@item dvbuffer
Set maximum size of buffer for incoming data, in frames. For DV, this
is an exact value. For HDV, it is not frame exact, since HDV does
not have a fixed frame size.

@item dvguid
Select the capture device by specifying its GUID. Capturing will only
be performed from the specified device and fails if no device with the
given GUID is found. This is useful to select the input if multiple
devices are connected at the same time.
Look at /sys/bus/firewire/devices to find out the GUIDs.

@end table

@subsection Examples

@itemize

@item
Grab and show the input of a FireWire DV/HDV device.
@example
ffplay -f iec61883 -i auto
@end example

@item
Grab and record the input of a FireWire DV/HDV device,
using a packet buffer of 100000 packets if the source is HDV.
@example
ffmpeg -f iec61883 -i auto -dvbuffer 100000 out.mpg
@end example

@end itemize

@section jack

JACK input device.

To enable this input device during configuration you need libjack
installed on your system.

A JACK input device creates one or more JACK writable clients, one for
each audio channel, with name @var{client_name}:input_@var{N}, where
@var{client_name} is the name provided by the application, and @var{N}
is a number which identifies the channel.
Each writable client will send the acquired data to the FFmpeg input
device.

Once you have created one or more JACK readable clients, you need to
connect them to one or more JACK writable clients.

To connect or disconnect JACK clients you can use the @command{jack_connect}
and @command{jack_disconnect} programs, or do it through a graphical interface,
for example with @command{qjackctl}.

To list the JACK clients and their properties you can invoke the command
@command{jack_lsp}.

Follows an example which shows how to capture a JACK readable client
with @command{ffmpeg}.
@example
# Create a JACK writable client with name "ffmpeg".
$ ffmpeg -f jack -i ffmpeg -y out.wav

# Start the sample jack_metro readable client.
$ jack_metro -b 120 -d 0.2 -f 4000

# List the current JACK clients.
$ jack_lsp -c
system:capture_1
system:capture_2
system:playback_1
system:playback_2
ffmpeg:input_1
metro:120_bpm

# Connect metro to the ffmpeg writable client.
$ jack_connect metro:120_bpm ffmpeg:input_1
@end example

For more information read:
@url{http://jackaudio.org/}

@subsection Options

@table @option

@item channels
Set the number of channels. Default is 2.

@end table

@section kmsgrab

KMS video input device.

Captures the KMS scanout framebuffer associated with a specified CRTC or plane as a
DRM object that can be passed to other hardware functions.

Requires either DRM master or CAP_SYS_ADMIN to run.

If you don't understand what all of that means, you probably don't want this.  Look at
@option{x11grab} instead.

@subsection Options

@table @option

@item device
DRM device to capture on.  Defaults to @option{/dev/dri/card0}.

@item format
Pixel format of the framebuffer.  This can be autodetected if you are running Linux 5.7
or later, but needs to be provided for earlier versions.  Defaults to @option{bgr0},
which is the most common format used by the Linux console and Xorg X server.

@item format_modifier
Format modifier to signal on output frames.  This is necessary to import correctly into
some APIs.  It can be autodetected if you are running Linux 5.7 or later, but will need
to be provided explicitly when needed in earlier versions.  See the libdrm documentation
for possible values.

@item crtc_id
KMS CRTC ID to define the capture source.  The first active plane on the given CRTC
will be used.

@item plane_id
KMS plane ID to define the capture source.  Defaults to the first active plane found if
neither @option{crtc_id} nor @option{plane_id} are specified.

@item framerate
Framerate to capture at.  This is not synchronised to any page flipping or framebuffer
changes - it just defines the interval at which the framebuffer is sampled.  Sampling
faster than the framebuffer update rate will generate independent frames with the same
content.  Defaults to @code{30}.

@end table

@subsection Examples

@itemize

@item
Capture from the first active plane, download the result to normal frames and encode.
This will only work if the framebuffer is both linear and mappable - if not, the result
may be scrambled or fail to download.
@example
ffmpeg -f kmsgrab -i - -vf 'hwdownload,format=bgr0' output.mp4
@end example

@item
Capture from CRTC ID 42 at 60fps, map the result to VAAPI, convert to NV12 and encode as H.264.
@example
ffmpeg -crtc_id 42 -framerate 60 -f kmsgrab -i - -vf 'hwmap=derive_device=vaapi,scale_vaapi=w=1920:h=1080:format=nv12' -c:v h264_vaapi output.mp4
@end example

@item
To capture only part of a plane the output can be cropped - this can be used to capture
a single window, as long as it has a known absolute position and size.  For example, to
capture and encode the middle quarter of a 1920x1080 plane:
@example
ffmpeg -f kmsgrab -i - -vf 'hwmap=derive_device=vaapi,crop=960:540:480:270,scale_vaapi=960:540:nv12' -c:v h264_vaapi output.mp4
@end example

@end itemize

@section lavfi

Libavfilter input virtual device.

This input device reads data from the open output pads of a libavfilter
filtergraph.

For each filtergraph open output, the input device will create a
corresponding stream which is mapped to the generated output.
The filtergraph is specified through the option @option{graph}.

@subsection Options

@table @option

@item graph
Specify the filtergraph to use as input. Each video open output must be
labelled by a unique string of the form "out@var{N}", where @var{N} is a
number starting from 0 corresponding to the mapped input stream
generated by the device.
The first unlabelled output is automatically assigned to the "out0"
label, but all the others need to be specified explicitly.

The suffix "+subcc" can be appended to the output label to create an extra
stream with the closed captions packets attached to that output
(experimental; only for EIA-608 / CEA-708 for now).
The subcc streams are created after all the normal streams, in the order of
the corresponding stream.
For example, if there is "out19+subcc", "out7+subcc" and up to "out42", the
stream #43 is subcc for stream #7 and stream #44 is subcc for stream #19.

If not specified defaults to the filename specified for the input
device.

@item graph_file
Set the filename of the filtergraph to be read and sent to the other
filters. Syntax of the filtergraph is the same as the one specified by
the option @var{graph}.

@item dumpgraph
Dump graph to stderr.

@end table

@subsection Examples

@itemize
@item
Create a color video stream and play it back with @command{ffplay}:
@example
ffplay -f lavfi -graph "color=c=pink [out0]" dummy
@end example

@item
As the previous example, but use filename for specifying the graph
description, and omit the "out0" label:
@example
ffplay -f lavfi color=c=pink
@end example

@item
Create three different video test filtered sources and play them:
@example
ffplay -f lavfi -graph "testsrc [out0]; testsrc,hflip [out1]; testsrc,negate [out2]" test3
@end example

@item
Read an audio stream from a file using the amovie source and play it
back with @command{ffplay}:
@example
ffplay -f lavfi "amovie=test.wav"
@end example

@item
Read an audio stream and a video stream and play it back with
@command{ffplay}:
@example
ffplay -f lavfi "movie=test.avi[out0];amovie=test.wav[out1]"
@end example

@item
Dump decoded frames to images and Closed Captions to an RCWT backup:
@example
ffmpeg -f lavfi -i "movie=test.ts[out0+subcc]" -map v frame%08d.png -map s -c copy -f rcwt subcc.bin
@end example

@end itemize

@section libcdio

Audio-CD input device based on libcdio.

To enable this input device during configuration you need libcdio
installed on your system. It requires the configure option
@code{--enable-libcdio}.

This device allows playing and grabbing from an Audio-CD.

For example to copy with @command{ffmpeg} the entire Audio-CD in @file{/dev/sr0},
you may run the command:
@example
ffmpeg -f libcdio -i /dev/sr0 cd.wav
@end example

@subsection Options
@table @option
@item speed
Set drive reading speed. Default value is 0.

The speed is specified CD-ROM speed units. The speed is set through
the libcdio @code{cdio_cddap_speed_set} function. On many CD-ROM
drives, specifying a value too large will result in using the fastest
speed.

@item paranoia_mode
Set paranoia recovery mode flags. It accepts one of the following values:

@table @samp
@item disable
@item verify
@item overlap
@item neverskip
@item full
@end table

Default value is @samp{disable}.

For more information about the available recovery modes, consult the
paranoia project documentation.
@end table

@section libdc1394

IIDC1394 input device, based on libdc1394 and libraw1394.

Requires the configure option @code{--enable-libdc1394}.

@subsection Options
@table @option

@item framerate
Set the frame rate. Default is @code{ntsc}, corresponding to a frame
rate of @code{30000/1001}.

@item pixel_format
Select the pixel format. Default is @code{uyvy422}.

@item video_size
Set the video size given as a string such as @code{640x480} or @code{hd720}.
Default is @code{qvga}.
@end table

@section openal

The OpenAL input device provides audio capture on all systems with a
working OpenAL 1.1 implementation.

To enable this input device during configuration, you need OpenAL
headers and libraries installed on your system, and need to configure
FFmpeg with @code{--enable-openal}.

OpenAL headers and libraries should be provided as part of your OpenAL
implementation, or as an additional download (an SDK). Depending on your
installation you may need to specify additional flags via the
@code{--extra-cflags} and @code{--extra-ldflags} for allowing the build
system to locate the OpenAL headers and libraries.

An incomplete list of OpenAL implementations follows:

@table @strong
@item Creative
The official Windows implementation, providing hardware acceleration
with supported devices and software fallback.
See @url{http://openal.org/}.
@item OpenAL Soft
Portable, open source (LGPL) software implementation. Includes
backends for the most common sound APIs on the Windows, Linux,
Solaris, and BSD operating systems.
See @url{http://kcat.strangesoft.net/openal.html}.
@item Apple
OpenAL is part of Core Audio, the official Mac OS X Audio interface.
See @url{http://developer.apple.com/technologies/mac/audio-and-video.html}
@end table

This device allows one to capture from an audio input device handled
through OpenAL.

You need to specify the name of the device to capture in the provided
filename. If the empty string is provided, the device will
automatically select the default device. You can get the list of the
supported devices by using the option @var{list_devices}.

@subsection Options

@table @option

@item channels
Set the number of channels in the captured audio. Only the values
@option{1} (monaural) and @option{2} (stereo) are currently supported.
Defaults to @option{2}.

@item sample_size
Set the sample size (in bits) of the captured audio. Only the values
@option{8} and @option{16} are currently supported. Defaults to
@option{16}.

@item sample_rate
Set the sample rate (in Hz) of the captured audio.
Defaults to @option{44.1k}.

@item list_devices
If set to @option{true}, print a list of devices and exit.
Defaults to @option{false}.

@end table

@subsection Examples

Print the list of OpenAL supported devices and exit:
@example
$ ffmpeg -list_devices true -f openal -i dummy out.ogg
@end example

Capture from the OpenAL device @file{DR-BT101 via PulseAudio}:
@example
$ ffmpeg -f openal -i 'DR-BT101 via PulseAudio' out.ogg
@end example

Capture from the default device (note the empty string '' as filename):
@example
$ ffmpeg -f openal -i '' out.ogg
@end example

Capture from two devices simultaneously, writing to two different files,
within the same @command{ffmpeg} command:
@example
$ ffmpeg -f openal -i 'DR-BT101 via PulseAudio' out1.ogg -f openal -i 'ALSA Default' out2.ogg
@end example
Note: not all OpenAL implementations support multiple simultaneous capture -
try the latest OpenAL Soft if the above does not work.

@section oss

Open Sound System input device.

The filename to provide to the input device is the device node
representing the OSS input device, and is usually set to
@file{/dev/dsp}.

For example to grab from @file{/dev/dsp} using @command{ffmpeg} use the
command:
@example
ffmpeg -f oss -i /dev/dsp /tmp/oss.wav
@end example

For more information about OSS see:
@url{http://manuals.opensound.com/usersguide/dsp.html}

@subsection Options

@table @option

@item sample_rate
Set the sample rate in Hz. Default is 48000.

@item channels
Set the number of channels. Default is 2.

@end table

@section pulse

PulseAudio input device.

To enable this output device you need to configure FFmpeg with @code{--enable-libpulse}.

The filename to provide to the input device is a source device or the
string "default"

To list the PulseAudio source devices and their properties you can invoke
the command @command{pactl list sources}.

More information about PulseAudio can be found on @url{http://www.pulseaudio.org}.

@subsection Options
@table @option
@item server
Connect to a specific PulseAudio server, specified by an IP address.
Default server is used when not provided.

@item name
Specify the application name PulseAudio will use when showing active clients,
by default it is the @code{LIBAVFORMAT_IDENT} string.

@item stream_name
Specify the stream name PulseAudio will use when showing active streams,
by default it is "record".

@item sample_rate
Specify the samplerate in Hz, by default 48kHz is used.

@item channels
Specify the channels in use, by default 2 (stereo) is set.

@item frame_size
This option does nothing and is deprecated.

@item fragment_size
Specify the size in bytes of the minimal buffering fragment in PulseAudio, it
will affect the audio latency. By default it is set to 50 ms amount of data.

@item wallclock
Set the initial PTS using the current time. Default is 1.

@end table

@subsection Examples
Record a stream from default device:
@example
ffmpeg -f pulse -i default /tmp/pulse.wav
@end example

@section sndio

sndio input device.

To enable this input device during configuration you need libsndio
installed on your system.

The filename to provide to the input device is the device node
representing the sndio input device, and is usually set to
@file{/dev/audio0}.

For example to grab from @file{/dev/audio0} using @command{ffmpeg} use the
command:
@example
ffmpeg -f sndio -i /dev/audio0 /tmp/oss.wav
@end example

@subsection Options

@table @option

@item sample_rate
Set the sample rate in Hz. Default is 48000.

@item channels
Set the number of channels. Default is 2.

@end table

@section video4linux2, v4l2

Video4Linux2 input video device.

"v4l2" can be used as alias for "video4linux2".

If FFmpeg is built with v4l-utils support (by using the
@code{--enable-libv4l2} configure option), it is possible to use it with the
@code{-use_libv4l2} input device option.

The name of the device to grab is a file device node, usually Linux
systems tend to automatically create such nodes when the device
(e.g. an USB webcam) is plugged into the system, and has a name of the
kind @file{/dev/video@var{N}}, where @var{N} is a number associated to
the device.

Video4Linux2 devices usually support a limited set of
@var{width}x@var{height} sizes and frame rates. You can check which are
supported using @command{-list_formats all} for Video4Linux2 devices.
Some devices, like TV cards, support one or more standards. It is possible
to list all the supported standards using @command{-list_standards all}.

The time base for the timestamps is 1 microsecond. Depending on the kernel
version and configuration, the timestamps may be derived from the real time
clock (origin at the Unix Epoch) or the monotonic clock (origin usually at
boot time, unaffected by NTP or manual changes to the clock). The
@option{-timestamps abs} or @option{-ts abs} option can be used to force
conversion into the real time clock.

Some usage examples of the video4linux2 device with @command{ffmpeg}
and @command{ffplay}:
@itemize
@item
List supported formats for a video4linux2 device:
@example
ffplay -f video4linux2 -list_formats all /dev/video0
@end example

@item
Grab and show the input of a video4linux2 device:
@example
ffplay -f video4linux2 -framerate 30 -video_size hd720 /dev/video0
@end example

@item
Grab and record the input of a video4linux2 device, leave the
frame rate and size as previously set:
@example
ffmpeg -f video4linux2 -input_format mjpeg -i /dev/video0 out.mpeg
@end example
@end itemize

For more information about Video4Linux, check @url{http://linuxtv.org/}.

@subsection Options

@table @option
@item standard
Set the standard. Must be the name of a supported standard. To get a
list of the supported standards, use the @option{list_standards}
option.

@item channel
Set the input channel number. Default to -1, which means using the
previously selected channel.

@item video_size
Set the video frame size. The argument must be a string in the form
@var{WIDTH}x@var{HEIGHT} or a valid size abbreviation.

@item pixel_format
Select the pixel format (only valid for raw video input).

@item input_format
Set the preferred pixel format (for raw video) or a codec name.
This option allows one to select the input format, when several are
available.

@item framerate
Set the preferred video frame rate.

@item list_formats
List available formats (supported pixel formats, codecs, and frame
sizes) and exit.

Available values are:
@table @samp
@item all
Show all available (compressed and non-compressed) formats.

@item raw
Show only raw video (non-compressed) formats.

@item compressed
Show only compressed formats.
@end table

@item list_standards
List supported standards and exit.

Available values are:
@table @samp
@item all
Show all supported standards.
@end table

@item timestamps, ts
Set type of timestamps for grabbed frames.

Available values are:
@table @samp
@item default
Use timestamps from the kernel.

@item abs
Use absolute timestamps (wall clock).

@item mono2abs
Force conversion from monotonic to absolute timestamps.
@end table

Default value is @code{default}.

@item use_libv4l2
Use libv4l2 (v4l-utils) conversion functions. Default is 0.

@end table

@section vfwcap

VfW (Video for Windows) capture input device.

The filename passed as input is the capture driver number, ranging from
0 to 9. You may use "list" as filename to print a list of drivers. Any
other filename will be interpreted as device number 0.

@subsection Options

@table @option

@item video_size
Set the video frame size.

@item framerate
Set the grabbing frame rate. Default value is @code{ntsc},
corresponding to a frame rate of @code{30000/1001}.

@end table

@section x11grab

X11 video input device.

To enable this input device during configuration you need libxcb
installed on your system. It will be automatically detected during
configuration.

This device allows one to capture a region of an X11 display.

The filename passed as input has the syntax:
@example
[@var{hostname}]:@var{display_number}.@var{screen_number}[+@var{x_offset},@var{y_offset}]
@end example

@var{hostname}:@var{display_number}.@var{screen_number} specifies the
X11 display name of the screen to grab from. @var{hostname} can be
omitted, and defaults to "localhost". The environment variable
@env{DISPLAY} contains the default display name.

@var{x_offset} and @var{y_offset} specify the offsets of the grabbed
area with respect to the top-left border of the X11 screen. They
default to 0.

Check the X11 documentation (e.g. @command{man X}) for more detailed
information.

Use the @command{xdpyinfo} program for getting basic information about
the properties of your X11 display (e.g. grep for "name" or
"dimensions").

For example to grab from @file{:0.0} using @command{ffmpeg}:
@example
ffmpeg -f x11grab -framerate 25 -video_size cif -i :0.0 out.mpg
@end example

Grab at position @code{10,20}:
@example
ffmpeg -f x11grab -framerate 25 -video_size cif -i :0.0+10,20 out.mpg
@end example

@subsection Options

@table @option
@item select_region
Specify whether to select the grabbing area graphically using the pointer.
A value of @code{1} prompts the user to select the grabbing area graphically
by clicking and dragging. A single click with no dragging will select the
whole screen. A region with zero width or height will also select the whole
screen. This option overwrites the @var{video_size}, @var{grab_x}, and
@var{grab_y} options. Default value is @code{0}.

@item draw_mouse
Specify whether to draw the mouse pointer. A value of @code{0} specifies
not to draw the pointer. Default value is @code{1}.

@item follow_mouse
Make the grabbed area follow the mouse. The argument can be
@code{centered} or a number of pixels @var{PIXELS}.

When it is specified with "centered", the grabbing region follows the mouse
pointer and keeps the pointer at the center of region; otherwise, the region
follows only when the mouse pointer reaches within @var{PIXELS} (greater than
zero) to the edge of region.

For example:
@example
ffmpeg -f x11grab -follow_mouse centered -framerate 25 -video_size cif -i :0.0 out.mpg
@end example

To follow only when the mouse pointer reaches within 100 pixels to edge:
@example
ffmpeg -f x11grab -follow_mouse 100 -framerate 25 -video_size cif -i :0.0 out.mpg
@end example

@item framerate
Set the grabbing frame rate. Default value is @code{ntsc},
corresponding to a frame rate of @code{30000/1001}.

@item show_region
Show grabbed region on screen.

If @var{show_region} is specified with @code{1}, then the grabbing
region will be indicated on screen. With this option, it is easy to
know what is being grabbed if only a portion of the screen is grabbed.

@item region_border
Set the region border thickness if @option{-show_region 1} is used.
Range is 1 to 128 and default is 3 (XCB-based x11grab only).

For example:
@example
ffmpeg -f x11grab -show_region 1 -framerate 25 -video_size cif -i :0.0+10,20 out.mpg
@end example

With @var{follow_mouse}:
@example
ffmpeg -f x11grab -follow_mouse centered -show_region 1 -framerate 25 -video_size cif -i :0.0 out.mpg
@end example

@item window_id
Grab this window, instead of the whole screen. Default value is 0, which maps to
the whole screen (root window).

The id of a window can be found using the @command{xwininfo} program, possibly with options -tree and
-root.

If the window is later enlarged, the new area is not recorded. Video ends when
the window is closed, unmapped (i.e., iconified) or shrunk beyond the video
size (which defaults to the initial window size).

This option disables options @option{follow_mouse} and @option{select_region}.

@item video_size
Set the video frame size. Default is the full desktop or window.

@item grab_x
@item grab_y
Set the grabbing region coordinates. They are expressed as offset from
the top left corner of the X11 window and correspond to the
@var{x_offset} and @var{y_offset} parameters in the device name. The
default value for both options is 0.
@end table

@c man end INPUT DEVICES
