---
title: "Infrastructure Cascade Analysis"
description: "Dependency graph modeling for critical infrastructure and undersea cable monitoring, visualizing how disruptions cascade across countries and systems."
---
Critical infrastructure is interdependent. A cable cut doesn't just affect connectivity; it creates cascading effects across dependent countries and systems. The cascade analysis and cable monitoring systems visualize these dependencies and provide early warning of disruptions.

## Dependency Graph

The system builds a graph of **350 infrastructure nodes** and dependency edges:

| Node Type | Count | Examples |
|-----------|-------|----------|
| **Undersea Cables** | 86 | MAREA, FLAG Europe-Asia, SEA-ME-WE 6 |
| **Pipelines** | 88 | Nord Stream, Trans-Siberian, Keystone |
| **Ports** | 62 | Singapore, Rotterdam, Shenzhen |
| **Chokepoints** | 9 | Suez, Hormuz, Malacca, Gibraltar, Bosphorus, Dardanelles |
| **Countries** | 105 | End nodes representing national impact |

## Cascade Calculation

When a user selects an infrastructure asset for analysis, a **breadth-first cascade** propagates through the graph:

```
1. Start at source node (e.g., "cable:marea")
2. For each dependent node:
   impact = edge_strength × disruption_level × (1 - redundancy)
3. Categorize impact:
   - Critical: impact > 0.8
   - High: impact > 0.5
   - Medium: impact > 0.2
   - Low: impact ≤ 0.2
4. Recurse to depth 3 (prevent infinite loops)
```

## Redundancy Modeling

The system accounts for alternative routes:

- Cables with high redundancy show reduced impact
- Countries with multiple cable landings show lower vulnerability
- Alternative routes are displayed with capacity percentages

## Example Analysis

**MAREA Cable Disruption**:
```
Source: MAREA (US ↔ Spain, 200 Tbps)
Countries Affected: 4
- Spain: Medium (redundancy via other Atlantic cables)
- Portugal: Low (secondary landing)
- France: Low (alternative routes via UK)
- US: Low (high redundancy)
Alternative Routes: TAT-14 (35%), Hibernia (22%), AEConnect (18%)
```

**FLAG Europe-Asia Disruption**:
```
Source: FLAG Europe-Asia (UK ↔ Japan)
Countries Affected: 7
- India: Medium (major capacity share)
- UAE, Saudi Arabia: Medium (limited alternatives)
- UK, Japan: Low (high redundancy)
Alternative Routes: SEA-ME-WE 6 (11%), 2Africa (8%), Falcon (8%)
```

## Use Cases

- **Pre-positioning**: Understand which countries are most vulnerable to specific infrastructure failures
- **Risk Assessment**: Evaluate supply chain exposure to chokepoint disruptions
- **Incident Response**: Quickly identify downstream effects of reported cable cuts or pipeline damage

## Undersea Cable Activity Monitoring

The dashboard monitors real-time cable operations and advisories from official maritime warning systems, providing early warning of potential connectivity disruptions.

### Backed by endpoints

| Method | Route | What it feeds |
|--------|-------|---------------|
| `GET` | `/api/infrastructure/v1/get-cable-health` | Cable health map/tooltips and cascade context. `fetchCableHealth()` calls this RPC when the cable layer is active, keeps a 1-minute local cache, and the server response is backed by Redis plus NGA warning analysis. |

### Data Sources

| Source | Coverage | Data Type |
|--------|----------|-----------|
| **NGA Warnings** | Global | NAVAREA maritime warnings |
| **Cable Operators** | Route-specific | Maintenance advisories |

### How It Works

The system parses NGA (National Geospatial-Intelligence Agency) maritime warnings for cable-related activity:

1. **Keyword filtering**: Warnings containing "CABLE", "CABLESHIP", "SUBMARINE CABLE", "FIBER OPTIC" are extracted
2. **Coordinate parsing**: DMS and decimal coordinates are extracted from warning text
3. **Cable matching**: Coordinates are matched to nearest cable routes within 5° radius
4. **Severity classification**: Keywords like "FAULT", "BREAK", "DAMAGE" indicate faults; others indicate maintenance

### Alert Types

| Type | Trigger | Map Display |
|------|---------|-------------|
| **Cable Advisory** | Any cable-related NAVAREA warning | Yellow marker at location |
| **Repair Ship** | Cableship name detected in warning | Ship icon with status |

### Repair Ship Tracking

When a cableship is mentioned in warnings, the system extracts:

- **Vessel name**: CS Reliance, Cable Innovator, etc.
- **Status**: "En route" or "On station"
- **Location**: Current working area
- **Associated cable**: Nearest cable route

This enables monitoring of ongoing repair operations before official carrier announcements.

### Why This Matters

Undersea cables carry 95% of intercontinental data traffic. A cable cut can:

- Cause regional internet outages
- Disrupt financial transactions
- Impact military communications
- Create economic cascading effects

Early visibility into cable operations, even maintenance windows, provides advance warning for contingency planning.
