# class RealTimeTransimissionStateListener

    interface RealTimeTransimissionStateListener

Package: | dji.v5.manager.aircraft.megaphone

##### Description:

Status listener for streaming mode.
`Supported since MSDK 5.0.0`

##### Class Members:

method
onProgress

###### method onProgress

    void onProgress(long sentBytes, long totalBytes)

Package: | dji.v5.manager.aircraft.megaphone

##### Description:

To get the transfer progress for streaming mode.
`Supported since MSDK 5.0.0`

##### Input Parameters:

long sentBytes | The number of bytes that have been transferred.
long totalBytes | The total number of bytes that need to be transferred.

method
onUploadedStatus

###### method onUploadedStatus

    void onUploadedStatus(UploadState uploadState)

Package: | dji.v5.manager.aircraft.megaphone

##### Description:

To get the transmission status of the streaming mode.
`Supported since MSDK 5.0.0`

##### Input Parameters:

UploadState uploadState | Transmission Status

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found