# class CameraStorageInfo

    class CameraStorageInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Details of the camera storage card. storage cards include: SD Card and onboard memory.

##### Class Members:

#### Members

method
getStorageType

###### method getStorageType

    CameraStorageLocation getStorageType()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get camera storage type.

##### Return:

CameraStorageLocation | Return camera storage type.

method
getStorageState

###### method getStorageState

    SDCardLoadState getStorageState()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Get the storage card insertion status. On-board memory is plugged in by default.

##### Return:

SDCardLoadState | Return the storage card inserted state.

method
getStorageCapacity

###### method getStorageCapacity

    Integer getStorageCapacity()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the storage card capacity. Unit: MB.

##### Return:

Integer | Return the storage card capacity.

method
getStorageLeftCapacity

###### method getStorageLeftCapacity

    Integer getStorageLeftCapacity()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the remaining capacity of the memory card. Unit: MB.

##### Return:

Integer | Return the remaining capacity of the memory card.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found