# class VideoRecordingStatus

    class VideoRecordingStatus implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Recroding status.

##### Class Members:

#### Members

method
getIsRecording

###### method getIsRecording

    Boolean getIsRecording()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets whether the camera is recording.

##### Return:

Boolean | Returns whether the camera is recording.

method
getIsPreRecording

###### method getIsPreRecording

    Boolean getIsPreRecording()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets whether the camera is pre-recording.

##### Return:

Boolean | Returns whether the camera is pre-recording.

method
getState

###### method getState

    VideoRecordingState getState()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Get camera recording status. When the status is `STARTING` and `STOPPING`, camera photo and video operations cannot be performed.

##### Return:

VideoRecordingState | Return to camera recording state.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found