# class PhotoIntervalShootSettings

    class PhotoIntervalShootSettings implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Setting of interval shooting parameter.

##### Class Members:

#### Members

method
getCount

###### method getCount

    Integer getCount()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get photo number of interval shooting.

##### Return:

Integer | Return photo number of interval shooting.

method
setCount

###### method setCount

    void setCount(Integer count)

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To set the photo number of interval shooting.

##### Input Parameters:

Integer count | Photo number of interval shooting that needs to be set.

method
getInterval

###### method getInterval

    Double getInterval()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To get the time of interval shopoting.

##### Return:

Double | Return the time of interval shopoting.

method
setInterval

###### method setInterval

    void setInterval(Double interval)

Package: | dji.sdk.keyvalue.value.camera

##### Description:

To set the time of interval shopoting.

##### Input Parameters:

Double interval | The time of interval shopoting that needs to be set.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found