# class LTEAuthenticationInfo

    @Keep
     class LTEAuthenticationInfo

Package: | dji.v5.manager.aircraft.lte

##### Description:

LTE authentication information. Including whether authenticated, the authenticated mobile phone number, the last authentication time and the remaining time of authentication.
`Supported since MSDK 5.2.0`

##### Class Members:

method
isLTEAuthenticationAvailable

###### method isLTEAuthenticationAvailable

    boolean isLTEAuthenticationAvailable()

Package: | dji.v5.manager.aircraft.lte

##### Description:

Gets whether the LTE authentication function is available.

##### Return:

boolean | `true` indicates that the LTE authentication feature is available.

method
isLTEAuthenticated

###### method isLTEAuthenticated

    boolean isLTEAuthenticated()

Package: | dji.v5.manager.aircraft.lte

##### Description:

Gets whether the drone is LTE authenticated.

##### Return:

boolean | `true` means the drone is LTE authenticated.

method
getLTEAuthenticatedPhoneAreaCode

###### method getLTEAuthenticatedPhoneAreaCode

    String getLTEAuthenticatedPhoneAreaCode()

Package: | dji.v5.manager.aircraft.lte

##### Description:

Gets the area code of the mobile phone number for this drone's LTE authentication.

##### Return:

String | Returns the area code of the mobile phone number for this drone's LTE authentication.

method
getLTEAuthenticatedPhoneNumber

###### method getLTEAuthenticatedPhoneNumber

    String getLTEAuthenticatedPhoneNumber()

Package: | dji.v5.manager.aircraft.lte

##### Description:

Gets the mobile phone number for LTE authentication of this drone.

##### Return:

String | Returns the mobile phone number for LTE authentication of this drone.

method
getLTELastAuthenticatedTime

###### method getLTELastAuthenticatedTime

    long getLTELastAuthenticatedTime()

Package: | dji.v5.manager.aircraft.lte

##### Description:

Gets the UTC timestamp of the last LTE authentication for this drone.

##### Return:

long | Returns the UTC timestamp of the last LTE authentication for this drone.

method
getLTEAuthenticatedRemainingTime

###### method getLTEAuthenticatedRemainingTime

    long getLTEAuthenticatedRemainingTime()

Package: | dji.v5.manager.aircraft.lte

##### Description:

Get the remaining UTC timestamp of this drone's LTE authentication. LTE authentication is valid for 30 days by default.

##### Return:

long | Returns the remaining UTC timestamp of this drone's LTE authentication.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found