# class FrequencyInterferenceInfo

    class FrequencyInterferenceInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.airlink

##### Description:

This class is used to get the information of frequency interference.

##### Class Members:

method
getFrequencyFrom

###### method getFrequencyFrom

    Double getFrequencyFrom()

Package: | dji.sdk.keyvalue.value.airlink

##### Description:

Get the start frequency.

##### Return:

Double | Return the start frequency.

method
getFrequencyTo

###### method getFrequencyTo

    Double getFrequencyTo()

Package: | dji.sdk.keyvalue.value.airlink

##### Description:

Get the stop frequency.

##### Return:

Double | Return the stop frequency.

method
getRssi

###### method getRssi

    Integer getRssi()

Package: | dji.sdk.keyvalue.value.airlink

##### Description:

Get the signal strength RSSI between the start and stop frequency. Unit is dBm.

##### Return:

Integer | Return the signal strength RSSI.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found