# class ZoomTargetPointInfo

    class ZoomTargetPointInfo implements DJIValue, JNIProguardKeepTag, ByteStream

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Point to focus information. The range of point focus coordinates x and y: [0,100]. [0,0] represents the upper left corner of the camera screen, and [100,100] represents the lower right corner of the camera screen. You only need to pass in the point and focus coordinates, other parameters are reserved fields and can be ignored.

##### Class Members:

#### Members

method
getX

###### method getX

    Double getX()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets the X-axis coordinate of the target point.

##### Return:

Double | Returns the X-axis coordinate of the target point.

method
getY

###### method getY

    Double getY()

Package: | dji.sdk.keyvalue.value.camera

##### Description:

Gets the Y-axis coordinate of the target point.

##### Return:

Double | Returns the Y-axis coordinate of the target point.

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found