<table>
    <tr>
        <td colspan="3"><center><b>Code Size of coreMQTT (example generated with GCC for ARM Cortex-M)</b></center></td>
    </tr>
    <tr>
        <td><b>File</b></td>
        <td><b><center>With -O1 Optimization</center></b></td>
        <td><b><center>With -Os Optimization</center></b></td>
    </tr>
    <tr>
        <td>core_mqtt.c</td>
        <td><center>8.3K</center></td>
        <td><center>7.2K</center></td>
    </tr>
    <tr>
        <td>core_mqtt_state.c</td>
        <td><center>1.7K</center></td>
        <td><center>1.3K</center></td>
    </tr>
    <tr>
        <td>core_mqtt_serializer.c</td>
        <td><center>9.5K</center></td>
        <td><center>7.3K</center></td>
    </tr>
    <tr>
        <td>core_mqtt_serializer_private.c</td>
        <td><center>0.8K</center></td>
        <td><center>0.7K</center></td>
    </tr>
    <tr>
        <td>core_mqtt_prop_serializer.c</td>
        <td><center>1.6K</center></td>
        <td><center>1.4K</center></td>
    </tr>
    <tr>
        <td>core_mqtt_prop_deserializer.c</td>
        <td><center>1.3K</center></td>
        <td><center>1.0K</center></td>
    </tr>
    <tr>
        <td><b>Total estimates</b></td>
        <td><b><center>23.2K</center></b></td>
        <td><b><center>18.9K</center></b></td>
    </tr>
</table>
