This technology file was generated using the Nano-CMOS tool from http://ptm.asu.edu/

The following default parameters were used:

NMOS
Leff=49 nm		10%
Vth=0.18 V		30mV
Vdd=1.3 V
Tox=1.6 nm
Rdsw=200 Ohm

PMOS
Leff=49 nm		10%
Vth=-0.18 V		30mV
Vdd=1.3 V
Tox=1.6 nm
Rdsw=240 Ohm