This technology file was generated using the Nano-CMOS tool from http://ptm.asu.edu/

The following default parameters were used:

NMOS
Leff=17.5 nm	10%
Vth=0.18 V		30mV
Vdd=1 V
Tox=1.1 nm
Rdsw=155 Ohm

PMOS
Leff=17.5 nm	10%
Vth=-0.18 V		30mV
Vdd=1 V
Tox=1.1 nm
Rdsw=155 Ohm