############################################
# Configuration file for running experiments
##############################################

# Path to directory of circuits to use
circuits_dir=benchmarks/titan_blif/titan23/stratixiv

# Path to directory of SDCs to use
sdc_dir=benchmarks/titan_blif/titan23/stratixiv

# Path to directory of architectures to use
archs_dir=arch/titan

# Add circuits to list to sweep
# Note that the circuits are roughly sorted so that some small
# circuits run first (to detect early failures), followed by larger
# circuits (so they do not start last)

#Largest benchmarks, which have potential to unroute or time-out
circuit_list_add=gaussianblur_stratixiv_arch_timing.blif 

#Large benchmarks
circuit_list_add=directrf_stratixiv_arch_timing.blif
circuit_list_add=bitcoin_miner_stratixiv_arch_timing.blif
circuit_list_add=LU230_stratixiv_arch_timing.blif
circuit_list_add=sparcT1_chip2_stratixiv_arch_timing.blif
circuit_list_add=LU_Network_stratixiv_arch_timing.blif

#Small benchmarks
circuit_list_add=neuron_stratixiv_arch_timing.blif
circuit_list_add=sparcT1_core_stratixiv_arch_timing.blif
circuit_list_add=stereo_vision_stratixiv_arch_timing.blif
circuit_list_add=cholesky_mc_stratixiv_arch_timing.blif

#Mixed order of large and small
circuit_list_add=gsm_switch_stratixiv_arch_timing.blif
circuit_list_add=mes_noc_stratixiv_arch_timing.blif
circuit_list_add=dart_stratixiv_arch_timing.blif
circuit_list_add=denoise_stratixiv_arch_timing.blif
circuit_list_add=sparcT2_core_stratixiv_arch_timing.blif
circuit_list_add=cholesky_bdti_stratixiv_arch_timing.blif
circuit_list_add=minres_stratixiv_arch_timing.blif
circuit_list_add=stap_qrd_stratixiv_arch_timing.blif
circuit_list_add=openCV_stratixiv_arch_timing.blif
circuit_list_add=bitonic_mesh_stratixiv_arch_timing.blif
circuit_list_add=segmentation_stratixiv_arch_timing.blif
circuit_list_add=SLAM_spheric_stratixiv_arch_timing.blif
circuit_list_add=des90_stratixiv_arch_timing.blif

# Add architectures to list to sweep
arch_list_add=stratixiv_arch.timing.xml

# Parse info and how to parse
parse_file=vpr_titan.txt

# How to parse QoR info
qor_parse_file=qor_vpr_titan.txt

# Pass requirements
pass_requirements_file=pass_requirements_vpr_titan.txt

#The Titan benchmarks are run at a fixed channel width of 300 to simulate a Stratix IV-like routing architecture
#A large number of routing iterations is set to ensure the router doesn't give up to easily on the larger benchmarks
#To be more run-time comparable to commercial tools like Quartus, we run with higher placer effort (inner_num=2) and lower astar_fac (1.0)
#Set a 48hr timeout so they don't run forever
script_params=-starting_stage vpr --route_chan_width 300 --max_router_iterations 400 --router_lookahead map --inner_num 2 --astar_fac 1.0 -timeout 172800
