# class INetworkRTKManager

    interface INetworkRTKManager

Package: | dji.v5.manager.interfaces

##### Description:

A class that manages network RTK, which is used to initialize and enable the chihiro network RTK, CMCC network RTK or custom network RTK service.
`Supported since MSDK 5.0.0`

##### Class Members:

method
setCustomNetworkRTKSettings

###### method setCustomNetworkRTKSettings

    void setCustomNetworkRTKSettings(RTKCustomNetworkSetting settings)

Package: | dji.v5.manager.interfaces

##### Description:

Configure the settings of custom network RTK.
`Supported since MSDK 5.0.0`

##### Input Parameters:

RTKCustomNetworkSetting settings | The settings of custom network RTK.

method
getCustomNetworkRTKSettings

###### method getCustomNetworkRTKSettings

    RTKCustomNetworkSetting getCustomNetworkRTKSettings()

Package: | dji.v5.manager.interfaces

##### Description:

Get the settings of custom network RTK.
`Supported since MSDK 5.0.0`

##### Return:

RTKCustomNetworkSetting | Return the settings of custom network RTK.

method
startNetworkRTKService

###### method startNetworkRTKService

    void startNetworkRTKService(CoordinateSystem coordinateSystem, final CommonCallbacks.CompletionCallback callback)

Package: | dji.v5.manager.interfaces

##### Description:

Start network RTK service.
`Supported since MSDK 5.0.0`

##### Input Parameters:

CoordinateSystem coordinateSystem | Network RTK coordinate system. This parameter only needs to be set when using Chihiro network RTK and CMCC network RTK. If it is not set, the default coordinate system of Chihiro network RTK is `CGCS2000`, and CMCC network RTK must set the coordinate system.
final CommonCallbacks.CompletionCallback callback | Return a result of the execution.

method
stopNetworkRTKService

###### method stopNetworkRTKService

    void stopNetworkRTKService(@NonNull final CommonCallbacks.CompletionCallback callback)

Package: | dji.v5.manager.interfaces

##### Description:

Stop network RTK service.
`Supported since MSDK 5.0.0`

##### Input Parameters:

@NonNull final CommonCallbacks.CompletionCallback callback | Return a result of the execution.

method
getNetworkRTKCoordinateSystem

###### method getNetworkRTKCoordinateSystem

    void getNetworkRTKCoordinateSystem(@NonNull final CommonCallbacks.CompletionCallbackWithParam<CoordinateSystem> callback)

Package: | dji.v5.manager.interfaces

##### Description:

Get the coordinate system of the network RTK.
`Supported since MSDK 5.0.0`

##### Input Parameters:

@NonNull final CommonCallbacks.CompletionCallbackWithParam<CoordinateSystem> callback | Return a result of the execution.

method
addNetworkRTKServiceInfoListener

###### method addNetworkRTKServiceInfoListener

    void addNetworkRTKServiceInfoListener(@NonNull final INetworkServiceInfoListener listener)

Package: | dji.v5.manager.interfaces

##### Description:

Add the listener of a network RTK service information.
`Supported since MSDK 5.0.0`

##### Input Parameters:

@NonNull final INetworkServiceInfoListener listener | The listener of a network RTK service information.

method
removeNetworkRTKServiceInfoListener

###### method removeNetworkRTKServiceInfoListener

    void removeNetworkRTKServiceInfoListener(@NonNull final INetworkServiceInfoListener listener)

Package: | dji.v5.manager.interfaces

##### Description:

Remove the listener of a network RTK service information.
`Supported since MSDK 5.0.0`

##### Input Parameters:

@NonNull final INetworkServiceInfoListener listener | The listener of a network RTK service information.

method
clearAllNetworkRTKServiceInfoListener

###### method clearAllNetworkRTKServiceInfoListener

    void clearAllNetworkRTKServiceInfoListener()

Package: | dji.v5.manager.interfaces

##### Description:

Remove all listeners of a network RTK service information.
`Supported since MSDK 5.0.0`

##### Related:

class
INetworkServiceInfoListener
class
RTKCustomNetworkSetting
enum
CoordinateSystem

###### enum CoordinateSystem

    enum  CoordinateSystem

Package: | dji.rtk

##### Description:

The coordinate system of the network RTK.
`Supported since MSDK 5.0.0`

##### Enum Members:

WGS84 | The World Geodetic System in 1984(WGS84).
CGCS2000 | China Geodetic Coordinate System in 2000(CGCS2000).

##### Class Members:

×

## Search Mobile SDK Document

{{searchCount}} Results

- ### {{{(item.highlights && item.highlights.title) || item.title}}}

  {{{(item.highlights && item.highlights.content[0]) || item.title}}}

Load More
Loading...
Not Found